For 1990-2009 cars

### Removal Procedure

1. Remove the turn signal multifunction switch. Refer to Turn Signal Multifunction Switch Replacement.
2. Remove the multifunction turn signal switch housing bolts.
3. Remove the multifunction turn signal switch housing.

### Installation Procedure

1. Install the multifunction turn signal switch housing.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the multifunction turn signal switch housing bolts.

Tighten
Tighten the bolts to 2.5 N·m (22 lb in).

3. Install the turn signal multifunction switch. Refer to Turn Signal Multifunction Switch Replacement.