For 1990-2009 cars

### Removal Procedure

1. Open the sunshade to the full open position.
2. Open the sunroof window to the full open position.

2.1. | Unhook the wind deflector slide blocks (1) from each side.

2.2. | Unhook the wind deflector tabs (2) from the rear of the upper frame.

2.3. | Remove the wind deflector.

### Installation Procedure

1. The window Must be in the full open position to do the following:

1.1. | Install the wind deflector to the upper frame.

1.2. | Hook the wind deflector slide blocks (1) to each side.

1.3. | Hook the wind deflector tabs (2) into the rear of the upper frame.

1.4. | Verify operation of the wind deflector.

2. Verify operations of the sunroof window.
3. Close the sunroof.