For 1990-2009 cars

Connector 1: | Engine Oil Pressure (EOP) Sensor
Connector 2: | Instrument Panel Cluster (IPC)

### Engine Oil Pressure (EOP) Sensor

#### Connector Part Information

- OEM: 12065400
- Service: 12126436
- Description: 4-Way F Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Engine Oil Pressure (EOP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN/BK | 231 | Oil Pressure Switch Signal
B | PU | 114 | Low Reference
C-D | -- | -- | Not Used

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 15364326
- Service: 89046871
- Description: 18-Way F Quadlok Micro (BK)

#### Terminal Part Information

- Pins: 1, 4, 5, 10, 11, 15, 16, 6, 7
- Terminal/Tray: 928999-5/15
- Core/Insulation Crimp: Pins 1, 4, 5, 10, 11, 15, 16 - H/H
- Core/Insulation Crimp: Pins 6, 7 - J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Instrument Panel Cluster (IPC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 1440 | Battery Positive Voltage
2-3 | -- | -- | Not Used
4 | BK/WH | 1151 | Ground
5 | BN/WH | 419 | MIL Control
6 | YE | 18 | Left Rear Turn Signal Lamps Supply Voltage
7 | D-GN | 19 | Right Rear Turn Signal Lamps Supply Voltage
8-9 | -- | -- | Not Used
10 | PU | 1807 | Class 2 Serial Data
11 | PU | 1807 | Class 2 Serial Data
12-14 | -- | -- | Not Used
15 | YE | 234 | Seat Belt Indicator Control
16 | GY | 728 | Security Indicator Control
17-18 | -- | -- | Not Used