For 1990-2009 cars

Figure 1: |

#### Driver Door

(1) | Door Lock Actuator - Driver
(2) | Door Lock and Window Switch - Driver
(3) | Speaker - LF Door Tweeter (UQ2)
(4) | Outside Rearview Mirror - Driver
(5) | Outside Rearview Mirror Switch
(6) | C202
(7) | C209
(8) | Speaker - LF Door
(9) | Window Motor - Driver
(10) | Inflatable Restraint Side Impact Sensor (SIS) - Left Connector (ASF)

Figure 2: |

#### Front Passenger Door

(1) | Outside Rearview Mirror - Front Passenger
(2) | Speaker - RF Door Tweeter (UQ2)
(3) | Door Lock and Window Switch - Front Passenger
(4) | Door Lock Actuator - Front Passenger
(5) | Inflatable Restraint Side Impact Sensor (SIS) - Right Connector (ASF)
(6) | Window Motor - Front Passenger
(7) | Speaker - RF Door
(8) | C211
(9) | C210

Figure 3: |

#### Left Rear Door (Crew Cab)

(1) | Speaker - LR Door
(2) | Door Lock and Window Switch - LR
(3) | C316
(4) | Window Motor - LR
(5) | Door Lock Actuator - LR

Figure 4: |

#### Right Rear Door (Crew Cab)

(1) | Door Lock and Window Switch - RR
(2) | Speaker - RR Door
(3) | Door Lock Actuator - RR
(4) | Window Motor - RR
(5) | C317