For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coolant Reservoir Bolt to Wheelhouse | 9 N·m | 81 lb in
Front Wiper Arm Nut | 33-38 N·m | 24-28 lb ft
Washer/Coolant Reservoir Bracket Bolts | 9 N·m | 81 lb in
Washer/Coolant Reservoir J-Clip Bolt | 9 N·m | 81 lb in
Washer Solvent Container to Fender Flange Bolts | 9 N·m | 81 lb in
Wiper Motor to Transmission Frame Bolts | 9 N·m | 81 lb in
Wiper Transmission Assembly to Cowl Panel Bolts | 9 N·m | 81 lb in