For 1990-2009 cars

Connector 1: | 1-2 Shift Solenoid (SS) Valve (M30)
Connector 2: | 2-3 Shift Solenoid (SS) Valve (M30)
Connector 3: | A/C Compressor Clutch (C60)
Connector 4: | A/C Refrigerant Pressure Sensor (C60)
Connector 5: | Accelerator Pedal Position (APP) Sensor
Connector 6: | Automatic Transmission Fluid Pressure (TFP) Manual Valve Position Switch (M30)
Connector 7: | Automatic Transmission Input Shaft Speed (ISS) Sensor (M30)
Connector 8: | Automatic Transmission Shift Lock Control Solenoid (M30)
Connector 9: | Ambient Light Sensor
Connector 10: | Accessory Power Outlet - I/P 1
Connector 11: | Accessory Power Outlet - I/P 2 (KC5)
Connector 12: | Backup Lamp - Left
Connector 13: | Backup Lamp - Right
Connector 14: | Backup Lamp Switch (MA5)
Connector 15: | Blower Motor
Connector 16: | Blower Motor Resistor Assembly
Connector 17: | Body Control Module (BCM) X1
Connector 18: | Body Control Module (BCM) X2
Connector 19: | Brake Fluid Level Switch
Connector 20: | Camshaft Position (CMP) Actuator Solenoid Valve
Connector 21: | Camshaft Position (CMP) Sensor (LH8)
Connector 22: | Camshaft Position (CMP) Sensor (LLR/LLV)
Connector 23: | Cargo Lamp - Left
Connector 24: | Cargo Lamp - Right
Connector 25: | Center High Mounted Stop Lamp (CHMSL) - Left
Connector 26: | Center High Mounted Stop Lamp (CHMSL) - Right
Connector 27: | Clutch Pedal Position (CPP) Sensor (MA5)
Connector 28: | Crankshaft Position (CKP) Sensor (LH8)
Connector 29: | Crankshaft Position (CKP) Sensor (LLR/LLV)
Connector 30: | Cruise Control Switch
Connector 31: | Data Link Connector (DLC)
Connector 32: | Data Link Resistor
Connector 33: | Digital Radio Receiver (U2K)
Connector 34: | Dome Lamp
Connector 35: | Door Jamb Switch - Driver
Connector 36: | Door Jamb Switch - Passenger
Connector 37: | Door Jamb Switch - Left Rear (Crew Cab)
Connector 38: | Door Jamb Switch - Right Rear (Crew Cab)
Connector 39: | Door Lock Actuator - Driver (AU3)
Connector 40: | Door Lock Actuator - Passenger (AU3)
Connector 41: | Door Lock Actuator - Left Rear (Crew Cab with AU3)
Connector 42: | Door Lock Actuator - Right Rear (Crew Cab with AU3)
Connector 43: | Door Lock/Window Switch - Driver X1 (A31/AU3)
Connector 44: | Door Lock/Window Switch - Driver X2 (A31/AU3)
Connector 45: | Door Lock/Window Switch - Passenger (A31/AU3)
Connector 46: | Electronic Brake Control Module (EBCM)
Connector 47: | Engine Control Module (ECM) X1
Connector 48: | Engine Control Module (ECM) X2
Connector 49: | Engine Control Module (ECM) X3
Connector 50: | Engine Coolant Temperature (ECT) Sensor (LH8)
Connector 51: | Engine Coolant Temperature (ECT) Sensor (LLR/LLV)
Connector 52: | Engine Oil Pressure (EOP) Sensor (LH8)
Connector 53: | Engine Oil Pressure (EOP) Switch (LLR/LLV)
Connector 54: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Connector 55: | Evaporative Emission (EVAP) Canister Vent Solenoid
Connector 56: | Evaporator Temperature Sensor (C60)
Connector 57: | Fog Lamp - Left Front (T96)
Connector 58: | Fog Lamp - Right Front (T96)
Connector 59: | Front Drive Axle Actuator (4WD)
Connector 60: | Fuel Injector 1 (LH8)
Connector 61: | Fuel Injector 1 (LLV)
Connector 62: | Fuel Injector 1 (LLR)
Connector 63: | Fuel Injector 2 (LH8)
Connector 64: | Fuel Injector 2 (LLV)
Connector 65: | Fuel Injector 2 (LLR)
Connector 66: | Fuel Injector 3 (LH8)
Connector 67: | Fuel Injector 3 (LLV)
Connector 68: | Fuel Injector 3 (LLR)
Connector 69: | Fuel Injector 4 (LH8)
Connector 70: | Fuel Injector 4 (LLV)
Connector 71: | Fuel Injector 4 (LLR)
Connector 72: | Fuel Injector 5 (LH8)
Connector 73: | Fuel Injector 5 (LLR)
Connector 74: | Fuel Injector 6 (LH8)
Connector 75: | Fuel Injector 7 (LH8)
Connector 76: | Fuel Injector 8 (LH8)
Connector 77: | Fuel Pump and Sender Assembly
Connector 78: | Fuel Pump Flow Control Module
Connector 79: | Fuel Tank Pressure (FTP) Sensor
Connector 80: | Generator X1
Connector 81: | Generator Battery Control Module
Connector 82: | Hazard Warning Switch
Connector 83: | Headlamp - Left High Beam (TT5)
Connector 84: | Headlamp - Right High Beam (TT5)
Connector 85: | Headlamp - Left (without TT5)
Connector 86: | Headlamp - Left Low Beam (TT5)
Connector 87: | Headlamp - Right Low Beam (TT5)
Connector 88: | Headlamp - Right (without TT5)
Connector 89: | Headlamp and Panel Dimmer Switch
Connector 90: | Heated Oxygen Sensor (HO2S) 1 (LLR/LLV)
Connector 91: | Heated Oxygen Sensor (HO2S) 2 (LLR/LLV)
Connector 92: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LH8)
Connector 93: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LH8)
Connector 94: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LH8)
Connector 95: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LH8)
Connector 96: | Heated Seat Element - Driver Back (KA1)
Connector 97: | Heated Seat Element - Passenger Back (KA1)
Connector 98: | Horn Assembly
Connector 99: | Horn Switch
Connector 100: | HVAC Control Module X1
Connector 101: | HVAC Control Module X2
Connector 102: | I/P Courtesy Lamp - Left
Connector 103: | I/P Courtesy Lamp - Right
Connector 104: | Ignition Coil 1 (LH8)
Connector 105: | Ignition Coil 1 (LLR/LLV)
Connector 106: | Ignition Coil 2 (LH8)
Connector 107: | Ignition Coil 2 (LLR/LLV)
Connector 108: | Ignition Coil 3 (LH8)
Connector 109: | Ignition Coil 3 (LLR/LLV)
Connector 110: | Ignition Coil 4 (LH8)
Connector 111: | Ignition Coil 4 (LLR/LLV)
Connector 112: | Ignition Coil 5 (LH8)
Connector 113: | Ignition Coil 5 (LLR)
Connector 114: | Ignition Coil 6 (LH8)
Connector 115: | Ignition Coil 7 (LH8)
Connector 116: | Ignition Coil 8 (LH8)
Connector 117: | Ignition Switch
Connector 118: | Inflatable Restraint Front End Sensor - Left
Connector 119: | Inflatable Restraint Front End Sensor - Right
Connector 120: | Inflatable Restraint I/P Module
Connector 121: | Inflatable Restraint Passenger Presence System (PPS) Module
Connector 122: | Inflatable Restraint Passenger Presence System (PPS) Sensor
Connector 123: | Inflatable Restraint Roof Rail Module - Left (ASF)
Connector 124: | Inflatable Restraint Roof Rail Module - Right (ASF)
Connector 125: | Inflatable Restraint Seat Position Sensor - Left
Connector 126: | Inflatable Restraint Seat Position Sensor - Right
Connector 127: | Inflatable Restraint Sensing and Diagnostic Module (SDM)
Connector 128: | Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)
Connector 129: | Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)
Connector 130: | Inflatable Restraint Steering Wheel Module X1
Connector 131: | Inflatable Restraint Steering Wheel Module X2
Connector 132: | Inside Rearview Mirror (ISRVM)
Connector 133: | Instrument Panel Cluster (IPC)
Connector 134: | Knock Sensor (KS) 1 (LH8)
Connector 135: | Knock Sensor (KS) 2 (LH8)
Connector 136: | Knock Sensor (KS) (LLR/LLV)
Connector 137: | License Lamp - Left
Connector 138: | License Lamp - Right
Connector 139: | Manifold Absolute Pressure (MAP) Sensor
Connector 140: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Connector 141: | Multifunction Switch - I/P
Connector 142: | Outside Rearview Mirror - Driver (DE6)
Connector 143: | Outside Rearview Mirror - Passenger (DE6)
Connector 144: | Outside Rearview Mirror Switch (DE6)
Connector 145: | Park Brake Switch
Connector 146: | Park/Neutral Position (PNP) Switch (M30)
Connector 147: | Park Lamp - Left Front
Connector 148: | Park Lamp - Right Front
Connector 149: | Park/Turn Signal Lamp - Left
Connector 150: | Park/Turn Signal Lamp - Right
Connector 151: | Pressure Control (PC) Solenoid Valve (M30)
Connector 152: | Radio X1
Connector 153: | Radio X2
Connector 154: | Recirculation Actuator (C60)
Connector 155: | Relay Inflatable Restraint
Connector 156: | Seat Adjuster Motor Assembly - Driver (AG1)
Connector 157: | Seat Adjuster Motor Assembly - Passenger (AG2)
Connector 158: | Seat Adjuster Switch - Driver X1 (AG1)
Connector 159: | Seat Adjuster Switch - Driver X2 (AG1)
Connector 160: | Seat Adjuster Switch - Passenger (AG2)
Connector 161: | Seat Belt Buckle - Driver
Connector 162: | Seat Belt Buckle - Passenger X1
Connector 163: | Seat Belt Buckle - Passenger X2
Connector 164: | Seat Belt Pretensioner - Driver
Connector 165: | Seat Belt Pretensioner - Passenger
Connector 166: | Seat Lumbar Adjuster Switch - Driver (AG1)
Connector 167: | Seat Lumbar Adjuster Switch - Passenger (AG2)
Connector 168: | Seat Lumbar Motor - Driver (AR9)
Connector 169: | Seat Lumbar Motor - Passenger (AR9)
Connector 170: | Seat Vertical Motor - Driver (AG1)
Connector 171: | Secondary Air Injection (AIR) Pump (K18)
Connector 172: | Secondary Air Injection (AIR) Pump Relay (K18)
Connector 173: | Secondary Air Injection (AIR) Pump Solenoid (K18)
Connector 174: | Speaker - Left Front
Connector 175: | Speaker - Left Front Tweeter (UQ2)
Connector 176: | Speaker - Left Rear (Extended/Crew Cab)
Connector 177: | Speaker - Right Front
Connector 178: | Speaker - Right Front Tweeter (UQ2)
Connector 179: | Speaker - Right Rear (Extended/Crew Cab)
Connector 180: | Starter X1
Connector 181: | Steering Wheel Position Sensor
Connector 182: | Stop Lamp Switch
Connector 183: | Stop Lamp - Left
Connector 184: | Stop Lamp - Right
Connector 185: | Sunroof Motor (CF5)
Connector 186: | Sunroof Switch (CF5)
Connector 187: | Throttle Body
Connector 188: | Theft Deterrent Module (TDM)
Connector 189: | Torque Converter Clutch (TCC) Solenoid Valve (M30)
Connector 190: | Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve (M30)
Connector 191: | Traction Control Switch
Connector 192: | Trailer Connector (UY7)
Connector 193: | Transfer Case Encoder Motor (4WD)
Connector 194: | Transfer Case 2/4 Wheel Indicator Switch (4WD)
Connector 195: | Transfer Case Neutral Switch (4WD)
Connector 196: | Transfer Case Shift Control Module X1 (4WD)
Connector 197: | Transfer Case Shift Control Module X2 (4WD)
Connector 198: | Transmission Control Module (TCM) (M30)
Connector 199: | Turn Signal Lamp - Left Rear
Connector 200: | Turn Signal Lamp - Right Rear
Connector 201: | Vehicle Communications Interface Module (VCIM) X1
Connector 202: | Vehicle Communications Interface Module (VCIM) X2
Connector 203: | Vehicle Speed Sensor (VSS)
Connector 204: | Window Switch - Left Rear (Crew Cab with A31)
Connector 205: | Window Switch - Right Rear (Crew Cab with A31)
Connector 206: | Wheel Speed Sensor (WSS) - Left Front
Connector 207: | Wheel Speed Sensor (WSS) - Right Front
Connector 208: | Window Motor - Driver (A31)
Connector 209: | Window Motor - Passenger (A31)
Connector 210: | Window Motor - Left Rear (Crew Cab A31)
Connector 211: | Window Motor - Right Rear (Crew Cab A31)
Connector 212: | Windshield Washer Fluid Pump
Connector 213: | Windshield Wiper Motor
Connector 214: | Yaw and Lateral Accelerometer Sensor (2WD) (JL4)
Connector 215: | Yaw and Lateral Accelerometer Sensor (4WD) (JL4)

### 1-2 Shift Solenoid (SS) Valve (M30)

#### Connector Part Information

- OEM: 12162201
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 P2 Series (NA)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### 1-2 Shift Solenoid (SS) Valve (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD | 839 | Ignition Voltage
B | 0.5 L-GN | 1222 | 1-2 Shift Solenoid Valve Control

### 2-3 Shift Solenoid (SS) Valve (M30)

#### Connector Part Information

- OEM: 12162201
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 P2 Series (NA)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### 2-3 Shift Solenoid (SS) Valve (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD | 839 | Ignition Voltage
B | 0.5 YE | 1223 | 2-3 Shift Solenoid Valve Control

### A/C Compressor Clutch (C60)

#### Connector Part Information

- OEM: 12162017
- Service: 12101937
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### A/C Compressor Clutch (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 350 | Ground
B | 0.35 D-GN | 59 | A/C Compressor Clutch Control

### A/C Refrigerant Pressure Sensor (C60)

#### Connector Part Information

- OEM: 13532244
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### A/C Refrigerant Pressure Sensor (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 2751 | Low Reference
2 | 0.35 GY | 2700 | 5-Volt Reference
3 | 0.35 RD/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 15383136
- Service: 89046653
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-969005-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-560/J-35616-33 (YE)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PU | 1272 | Low Reference
2 | 0.35 WH/BK | 1164 | 5-Volt Reference
3 | 0.35 D-BU | 1161 | APP Sensor 1 Signal
4 | 0.35 BN | 1271 | Low Reference
5 | 0.35 TN | 1274 | 5-Volt Reference
6 | 0.35 L-BU | 1162 | APP Sensor 2 Signal

### Automatic Transmission Fluid Pressure (TFP) Manual Valve Position Switch (M30)

#### Connector Part Information

- OEM: 12162213
- Service: Non-Serviceable
- Description: 5-Way F Metri-Pack 150.2 P2 Series (NA)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Automatic Transmission Fluid Pressure (TFP) Manual Valve Position Switch (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 1227 | TFT Sensor Signal
B | 0.5 GY | 452 | Low Reference
C | 0.5 PK | 1224 | Transmission Fluid Pressure Switch Signal A
D | 0.5 OG | 1226 | Transmission Fluid Pressure Switch Signal C
E | 0.5 D-BU | 1225 | Transmission Fluid Pressure Switch Signal B

### Automatic Transmission Input Shaft Speed (ISS) Sensor (M30)

#### Connector Part Information

- OEM: 15492436
- Service: Non-Serviceable
- Description: 3-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Automatic Transmission Input Shaft Speed (ISS) Sensor (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 1230 | ISS Signal
B | 0.5 RD | 839 | Ignition Voltage
C | 0.5 D-GN | 1231 | Low Reference

### Automatic Transmission Shift Lock Control Solenoid (M30)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Automatic Transmission Shift Lock Control Solenoid (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 323 | Shift Solenoid Control
B | 0.35 D-BU | 2050 | Ground

### Ambient Light Sensor

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ambient Light Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 278 | Ambient Light Sensor Signal
B | 0.35 BK | 279 | Low Reference

### Accessory Power Outlet - I/P 1

#### Connector Part Information

- OEM: 12176446
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series Flex Lock (BK)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - I/P 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 40 | Battery Positive Voltage
B | -- | -- | Not Used
C | 0.8 BK | 2050 | Ground

### Accessory Power Outlet - I/P 2 (KC5)

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series Flex Lock (BK)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: C
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - I/P 2 (KC5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 240 | Battery Positive Voltage
B | -- | -- | Not Used
C | 0.8 BK | 2050 | Ground

### Backup Lamp - Left

#### Connector Part Information

- OEM: 16530668
- Service: See Catalog
- Description: 3-Way F (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Backup Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN | -- | Backup Lamp Control
B | -- | -- | Not Used
G | BK | -- | Ground
BK | -- | Ground

### Backup Lamp - Right

#### Connector Part Information

- OEM: 16530668
- Service: See Catalog
- Description: 3-Way F (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Backup Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN | -- | Backup Lamp Control
B | -- | -- | Not Used
G | BK | -- | Ground
BK | -- | Ground

### Backup Lamp Switch (MA5)

#### Connector Part Information

- OEM: 12103584
- Service: 12085485
- Description: 2-Way M Weather-Pack (BK)

#### Terminal Part Information

- Terminal/Tray: See 12089040/3
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 12014012-1/J-35616-9 (OG)

#### Backup Lamp Switch (MA5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 539 | Ignition Voltage
B | 0.5 L-GN | 24 | Backup Lamp Control

### Blower Motor

#### Connector Part Information

- OEM: 15438389
- Service: 88987963
- Description: 2-Way F (WH)

#### Terminal Part Information

- Terminal/Tray: 7116-2877/10
- Core/Insulation Crimp: F/G
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BN | 41 | Ignition Voltage
2 | 2 OG | 52 | Blower Motor High Control

### Blower Motor Resistor Assembly

#### Connector Part Information

- OEM: 12129566
- Service: 15306069
- Description: 4-Way F Metri-Pack 280 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12015858/4
- Core/Insulation Crimp: F/G
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Blower Motor Resistor Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 TN | 63 | Blower Motor Medium 1 Control
B | 2 L-BU | 72 | Medium 2 Blower Motor Control
C | 2 OG | 52 | Blower Motor High Control
D | 2 YE | 60 | Blower Motor Low Control

### Body Control Module (BCM) X1

#### Connector Part Information

- OEM: 15480437
- Service: 88988604
- Description: 56-Way F GT 280/Micro 64 Series (BK)

#### Terminal Part Information

- Pins: A2, A3, A4, A5, A6, A7, A8, A11, A12, A18, A19, A20, A24, A25, A26, A29, A30, A31, A32, A38, A39, A40, A41, A42, A43, A44, A45, A46, A47, A48, B1, B2, B3, B4, B5, B6, B7, B8
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module (BCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.35 PK | 39 | Ignition 1 Voltage
A2 | 0.35 YE | 317 | Fog Lamp Relay Control
A3 | 0.8 L-BU | 14 | Left Turn Signal Lamps Control
A4 | 0.35 GY/BK | 690 | Courtesy Lamp Control (TR9)
A5 | 0.35 PK/WH | 1970 | Headlamp Relay Control
A6 | 0.35 BK | 755 | RAP Relay Coil Control
A7 | 0.5 OG | 740 | Battery Positive Voltage
A8 | 0.35 D-GN | 113 | Windshield Wiper Switch Signal 2
A9-A10 | -- | -- | Not Used
A11 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Control (AUO)
A12 | 0.35 WH | 194 | Door Unlock Control (AUO)
A13-A17 | -- | -- | Not Used
A18 | 0.35 BK/WH | 1969 | Beam Select Relay Control
A19 | 0.8 D-BU | 15 | Right Turn Signal Lamps Control
A20 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
A21-A23 | -- | -- | Not Used
A24 | 0.35 BN/WH | 301 | Park Lamp Relay Control
A25 | 0.35 BK/WH | 1524 | Seat Belt Switch - Left
A26 | 0.35 OG | 300 | Ignition Voltage
A27-A28 | -- | -- | Not Used
A29 | 0.35 OG | 1732 | Courtesy Lamps Control
A30 | 0.35 OG | 1732 | Courtesy Lamps Control
A31 | 0.8 L-BU | 1134 | Park Brake Switch Signal
A32 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
A33-A35 | -- | -- | Not Used
A36 | 0.35 PU | 544 | DRL Relay Control
A37 | -- | -- | Not Used
A38 | 0.35 L-GN/BK | 748 | Right Rear Door Ajar Switch Signal
A39 | 0.35 BK/WH | 746 | Right Rear Door Ajar Switch Signal (CREW CAB)
A40 | 0.35 BK | 28 | Horn Relay Control
A41 | 0.35 PU | 1807 | Class 2 Serial Data (UE1)
A42 | 0.35 PU | 1807 | Class 2 Serial Data
A43 | 0.35 D-GN/WH | 762 | A/C Request Signal
A44 | 0.35 L-BU/BK | 747 | Left Rear Door Ajar Switch Signal (CREW CAB)
A45 | 0.35 PK | 849 | Brake Fluid Level Sensor Signal
A46 | 0.35 WH | 156 | Courtesy Lamp Low Control
A47 | 0.35 PU | 1807 | Class 2 Serial Data
A48 | 0.35 BN | 9 | Park Lamp Control
B1 | 0.5 YE | 18 | Left Rear Turn Signal Lamps Control
B2 | 0.5 D-GN | 19 | Right Rear Turn Signal Lamps Control
B3 | 0.35 BK/WH | 1251 | Ground
B4 | 0.5 RD | 228 | Windshield Washer Pump Control
B5 | 0.5 OG | 840 | Battery Positive Voltage
B6 | 0.5 D-BU | 338 | Ignition Voltage
B7 | 0.5 BN | 4 | Ignition Voltage
0.5 BN | 4 | Ignition Voltage
B8 | 0.5 OG | 1340 | Battery Positive Voltage

### Body Control Module (BCM) X2

#### Connector Part Information

- OEM: 15480439
- Service: 88988604
- Description: 56-Way F GT 280/Micro 64 Series (GY)

#### Terminal Part Information

- Pins: A1, A2, A3, A4, A5, A7, A8, A9, A10, A11, A12, A13, A14, A17, A18, A19, A25, A26, A28, A29, A31, A35, A36, A37, A38, A39, A40, A41, A42, A43, A44, A45, A46, A47, A48, B3, B4, B5, B7, B8
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module (BCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
A2 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
A3 | 0.35 GY | 112 | Windshield Wiper Switch Signal 1
A4 | 0.5 BN/WH | 230 | Instrument Panel Lamps Dimming Control
A5 | 0.35 YE | 183 | Front Fog Lamp Indicator Control
A6 | -- | -- | Not Used
A7 | 0.35 BN/WH | 301 | Park Lamp Relay Control
A8 | 0.35 BN | 1356 | Flash To Pass Switch Signal
A9 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
A10 | 0.35 PU | 719 | Low Reference
A11 | 0.35 D-BU/WH | 1495 | Dome Overide Switch Signal
A12 | 0.35 PU | 328 | Interior Lamp Switch Signal
A13 | 0.35 WH/BK | 158 | Cargo Lamp Switch Signal (TR9)
A14 | 0.5 WH | 1390 | Ignition Voltage
A15-A16 | -- | -- | Not Used
A17 | 0.35 BN/WH | 1571 | Traction Control Switch Signal (2WD with NW7)
A18 | 0.35 OG | 192 | Fog Lamps Enable (T96)
A19 | 0.35 GY | 728 | Security Indicator Control
A20-A24 | -- | -- | Not Used
A25 | 0.35 BK | 28 | Horn Relay Control
A26 | 0.35 PU/WH | 1572 | TCS Requested Indicator Control (2WD with NW7)
A27 | -- | -- | Not Used
A28 | 0.35 GY | 8 | Instrument Panel Lamps Dimmer Switch Signal
A29 | 0.35 GY | 8 | Instrument Panel Lamps Dimmer Switch Signal
A30 | -- | -- | Not Used
A31 | 0.35 BN | 323 | Shift Solenoid Control
A32 | 0.35 PK | 2216 | A/C Recirculation Request Signal
A33-A34 | -- | -- | Not Used
A35 | 0.35 GY | 8 | Instrument Panel Lamp Dimmer Switch Signal
A36 | 0.35 GY | 8 | Instrument Panel Lamp Dimmer Switch Signal
A37 | 0.35 WH | 278 | Ambient Light Sensor Signal
A38 | 0.35 PU | 1807 | Class 2 Serial Data
A39 | 0.35 PU | 1807 | Class 2 Serial Data
A40 | 0.35 OG | 1732 | Courtesy Lamps Control (TR9)
A41 | 0.35 WH | 156 | Courtesy Lamp Low Control (TR9)
A42 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal
A43 | 0.35 BK | 279 | Low Reference
A44 | 0.35 PU | 1807 | Class 2 Serial Data
A45 | 0.35 L-BU | 1508 | Turn Signal Switch Signal
A46 | 0.35 OG | 1732 | Courtesy Lamps Control (TR9)
A47 | 0.35 WH | 156 | Courtesy Lamp Low Control (TR9)
A48 | 0.35 WH | 111 | Hazard Switch Signal
B1-B2 | -- | -- | Not Used
B3 | 0.5 D-GN | 19 | Right Rear Turn Signal Lamps Control
B4 | 0.5 YE | 18 | Left Rear Turn Signal Lamps Control
B5 | 0.5 RD | 228 | Windshield Washer Pump Control
B6 | -- | -- | Not Used
B7 | 0.5 BN | 4 | Ignition Voltage
B8 | 0.5 D-BU | 338 | Ignition Voltage
0.35 D-BU | 338 | Ignition Voltage

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: 15449028
- Service: 88987993
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 849 | Brake Fluid Level Sensor Signal
B | 0.35 BK | 850 | Ground

### Camshaft Position (CMP) Actuator Solenoid Valve

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See 15326427/5
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: See Terminal Repair Kit 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Actuator Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BN | 2198 | Camshaft Position Actuator Solenoid High Control
B | 0.35 BK | 2199 | Low Reference

### Camshaft Position (CMP) Sensor (LH8)

#### Connector Part Information

- OEM: 12059595
- Service: 88986451
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-BU | 6259 | 12-Volt Reference
B | 0.35 OG | 6260 | Low Reference
C | 0.35 D-BU/WH | 6265 | Camshaft Position Signal

### Camshaft Position (CMP) Sensor (LLR/LLV)

#### Connector Part Information

- OEM: 15393906
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 RD | 631 | 12-Volt Reference
B | 0.35 PK/BK | 632 | Low Reference
C | 0.35 BK | 630 | Camshaft Position Signal

### Cargo Lamp - Left

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F LP SOC Wedge Base Assembly (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Cargo Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 690 | Courtesy Lamps Control
0.35 WH | 690 | Courtesy Lamps Control
B | 0.35 BK/WH | 850 | Ground
0.35 BK/WH | 850 | Ground

### Cargo Lamp - Right

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F LP SOC Wedge Base Assembly (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Cargo Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 690 | Courtesy Lamps Control
B | 0.35 BK/WH | 850 | Ground

### Center High Mounted Stop Lamp (CHMSL) - Left

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F LP SOC Wedge Base Assembly (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Center High Mounted Stop Lamp (CHMSL) - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 20 | Stop Lamps Control
0.8 BN | 20 | Stop Lamps Control
B | 0.5 BK/WH | 850 | Ground
0.5 BK/WH | 850 | Ground

### Center High Mounted Stop Lamp (CHMSL) - Right

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F LP SOC Wedge Base Assembly (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Center High Mounted Stop Lamp (CHMSL) - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 20 | Stop Lamps Control
B | 0.5 BK/WH | 850 | Ground
0.5 BK/WH | 850 | Ground

### Clutch Pedal Position (CPP) Sensor (MA5)

#### Connector Part Information

- OEM: 15332132
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15393150/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Clutch Pedal Position (CPP) Sensor (MA5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 6293 | 5-Volt Reference
B | 0.35 D-BU | 6306 | Clutch Pedal Position Sensor Signal
C | 0.35 D-GN/WH | 6294 | Low Reference

### Crankshaft Position (CKP) Sensor (LH8)

#### Connector Part Information

- OEM: 12129946
- Service: 88987997
- Description: 3-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Crankshaft Position (CKP) Sensor (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH/BK | 6271 | CKP Sensor Signal
B | 0.5 GY/BK | 6272 | Low Reference
C | 0.5 PU/WH | 6270 | 5-Volt Reference

### Crankshaft Position (CKP) Sensor (LLR/LLV)

#### Connector Part Information

- OEM: 15393906
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Crankshaft Position (CKP) Sensor (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN | 1867 | 12-Volt Reference
B | 0.35 D-BU/WH | 1869 | CKP Sensor Signal
C | 0.35 YE/BK | 1868 | Low Reference

### Cruise Control Switch

#### Connector Part Information

- OEM: 15434331
- Service: 89046651
- Description: 2-Way F 250 58M (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-2875/10
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Cruise Control Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PK | 339 | Ignition Voltage
2 | 0.35 PU | 420 | TCC Brake Switch/Cruise Control Release Signal
0.35 PU | 420 | TCC Brake Switch/Cruise Control Release Signal

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 15317575
- Service: 15317575
- Description: 16-Way F Metri-Pack/150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12129484/19
- Core/Insulation Crimp: Pins 2, 4, 5 - E/C
- Core/Insulation Crimp: Pins 16 - E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 PU | 1807 | Class 2 Serial Data
3 | -- | -- | Not Used
4 | 0.35 BK | 2050 | Ground
5 | 0.35 BK/WH | 1151 | Ground
6 | 0.5 TN/WH | 2500 | High Speed GMLAN Serial Data (-)
7-13 | -- | -- | Not Used
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data (+)
15 | -- | -- | Not Used
16 | 0.8 OG | 40 | Battery Positive Voltage

### Data Link Resistor

#### Connector Part Information

- OEM: 13510085
- Service: See Catalog
- Description:2-Way F GT150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15326427/5
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Data Link Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 2500 | High Speed GMLAN Serial Data Bus +
B | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus -

### Digital Radio Receiver (U2K)

#### Connector Part Information

- OEM: 13567854
- Service: See Catalog
- Description: 16-Way F ASM (WH)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Digital Radio Receiver (U2K)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN/WH | 367 | Remote Playback Device Left Audio Signal
3 | 0.35 D-GN/WH | 368 | Remote Playback Device Right Audio Signal
4-6 | -- | -- | Not Used
7 | 0.35 PU | 1807 | Class 2 Serial Data
8 | -- | -- | Not Used
9 | 0.5 BK/WH | 1151 | Ground
10 | 0.35 BK/WH | 372 | Remote Playback Device Audio Common Signal
11-15 | -- | -- | Not Used
16 | 1 OG | 1140 | Battery Positive Voltage

### Dome Lamp

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Dome Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 1732 | Courtesy Lamps Control
B | 0.35 WH | 156 | Courtesy Lamp Low Control

### Door Jamb Switch - Driver

#### Connector Part Information

- OEM: 15316639
- Service: 15306434
- Description: 2-Way F Multi-Lock (BK)

#### Terminal Part Information

- Terminal/Tray: 173681-2/17
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Door Jamb Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
2 | 0.35 BK/WH | 1151 | Ground

### Door Jamb Switch - Passenger

#### Connector Part Information

- OEM: 15316639
- Service: 15306434
- Description: 2-Way F Multi-Lock (BK)

#### Terminal Part Information

- Terminal/Tray: 173681-2/17
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Door Jamb Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN/BK | 748 | Right Front Door Ajar Switch Signal
2 | 0.35 BK/WH | 1251 | Ground

### Door Jamb Switch - Left Rear (Crew Cab)

#### Connector Part Information

- OEM: 15316639
- Service: 15306434
- Description: 2-Way F Multi-Lock (BK)

#### Terminal Part Information

- Terminal/Tray: 173681-2/17
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Door Jamb Switch - Left Rear (Crew Cab)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 746 | Left Rear Door Ajar Switch Signal
2 | 0.35 BK/WH | 1251 | Ground

### Door Jamb Switch - Right Rear (Crew Cab)

#### Connector Part Information

- OEM: 15316639
- Service: 15306434
- Description: 2-Way F Multi-Lock (BK)

#### Terminal Part Information

- Terminal/Tray: 173681-2/17
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Door Jamb Switch - Right Rear (Crew Cab)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU/BK | 747 | Right Rear Door Ajar Switch Signal
2 | 0.35 BK/WH | 1151 | Ground

### Door Lock Actuator - Driver (AU3)

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 TN | 694 | Door Lock Actuator Unlock Control
2 | 0.8 GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Passenger (AU3)

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 TN | 294 | Door Lock Actuator Unlock Control
2 | 0.8 GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Left Rear (Crew Cab with AU3)

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Left Rear (Crew Cab with AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 TN | 294 | Door Lock Actuator Unlock Control
2 | 0.8 GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Right Rear (Crew Cab with AU3)

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Right Rear (Crew Cab with AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 TN | 294 | Door Lock Actuator Unlock Control
2 | 0.8 GY | 295 | Door Lock Actuator Lock Control

### Door Lock/Window Switch - Driver X1 (A31/AU3)

#### Connector Part Information

- OEM: 12105465
- Service: 88987940
- Description: 8-Way F 090 II (WH)

#### Terminal Part Information

- Pins: 1, 2, 3, 4, 5, 6, 7, 8
- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 1, 2, 3, 4, 5 - C/A
- Core/Insulation Crimp: Pins 6, 7, 8 - See Terminal Repair Kit
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Door Lock/Window Switch - Driver X1 (A31/AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 OG | 1240 | Battery Positive Voltage
2 | 0.8 TN | 694 | Driver Door Lock Actuator Unlock Control
3 | 0.5 BK | 850 | Ground
4 | 0.8 GY | 295 | Door Lock Actuator Lock Control
5 | 0.8 TN | 294 | Door Lock Actuator Unlock Control
6 | 2 YE | 443 | Ignition Voltage
7 | 2 D-BU | 164 | Power Window Motor Left Front Up Control
8 | 2 BN | 165 | Power Window Motor Left Front Down Control

### Door Lock/Window Switch - Driver X2 (A31/AU3)

#### Connector Part Information

- OEM: 15380363
- Service: 15380363
- Description: 14-Way F 040 III (WH)

#### Terminal Part Information

- Terminal/Tray: 15355438/20
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-12 (BU)

#### Door Lock/Window Switch - Driver X2 (A31/AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal
2 | 0.35 BN | 9 | Park Lamp Control
3 | -- | -- | Not Used
4 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal
5 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal
6 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Control
7 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Control
8 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal
9 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal
10 | -- | -- | Not Used
11 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal
12 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
13 | 0.35 WH | 194 | Door Unlock Control
14 | -- | -- | Not Used

### Door Lock/Window Switch - Passenger (A31/AU3)

#### Connector Part Information

- OEM: 15383359
- Service: 15383359
- Description: 12-Way F 090 II (WH)

#### Terminal Part Information

- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 3, 4, 6, 7, 8, 9, 10, 11, 12 - See Terminal Repair Kit
- Core/Insulation Crimp: Pins 5 - C/A
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Door Lock/Window Switch - Passenger (A31/AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Control
4 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Control
5 | 1 BK | 2050 | Ground
6 | 0.35 BN | 9 | Park Lamp Control
7 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal
8 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal
9 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal
10 | 2 BN | 667 | Power Window Motor Right Front Down Control
11 | 2 YE | 443 | Ignition Voltage
12 | 2 D-BU | 666 | Power Window Motor Right Front Up Control

### Electronic Brake Control Module (EBCM)

#### Connector Part Information

- OEM: 13580973
- Service: 19153161
- Description:47-Way F MK25/60 Series Sealed (BK)

#### Terminal Part Information

- Pins: 1, 16, 32
- Terminal/Tray:7116-4142-02/10
- Core/Insulation Crimp: A/3
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 5-9, 11, 12, 14, 18, 19, 22, 29, 30, 35, 40, 41, 45
- Terminal/Tray: 638551-1/16
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

- Pins: 33, 34, 36-38, 42, 43, 46
- Terminal/Tray: 638551-1/16
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Electronic Brake Control Module (EBCM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 RD | 542 | Battery Positive Voltage
2-4 | -- | -- | Not Used
5 | 0.35 GY | 1056 | Steering Wheel Position Sensor 5-Volt Reference
6 | 0.35 PU | 420 | Cruise Control Release Signal
7 | 0.35 TN | 464 | Delivered Torque Signal
8 | 0.35 BN | 441 | Ignition Voltage
9 | 0.35 L-BU | 1764 | Steering Wheel Position Signal B
10 | -- | -- | Not Used
11 | 0.35 PU | 1807 | Class 2 Serial Data
12 | 0.35 PU | 1807 | Class 2 Serial Data
13 | -- | -- | Not Used
14 | 0.35 OG/BK | 463 | Requested Torque Signal
15 | -- | -- | Not Used
16 | 3 BK | 850 | Ground
17 | -- | -- | Not Used
18 | 0.35 D-BU | 716 | CAN HI
19 | 0.35 L-BU | 2088 | CAN LO
20-21 | -- | -- | Not Used
22 | 0.35 GY/BK | 1337 | Ignition Voltage
23-28 | -- | -- | Not Used
29 | 0.35 OR/BK | 1057 | Ground
30 | 0.35 L-BU | 1059 | Steering Wheel Position Sensor Signal
31 | -- | -- | Not Used
32 | 2 OR | 540 | Battery Positive Voltage
33 | 0.5 TN | 833 | Low Reference
34 | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
35 | 0.35 TN | 848 | ABS Brake Switch Signal
36 | 0.5 BK | 884 | Left Rear Wheel Speed Sensor Signal
37 | 0.5 RD | 885 | Low Reference
38 | 0.35 WH | 1765 | Steering Wheel Position Marker Pulse Signal
39 | -- | -- | Not Used
40 | 0.35 BK | 1835 | Low Reference
41 | 0.35 L-GN | 1763 | Steering Wheel Position Signal A
42 | 0.5 WH | 883 | Low Reference
43 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
44 | -- | -- | Not Used
45 | 0.35 L-BU | 830 | 12-Volt Reference
46 | 0.5 YE | 873 | Left Front Wheel Speed Sensor Signal
47 | -- | -- | Not Used

### Engine Control Module (ECM) X1

#### Connector Part Information

- OEM: 13599443
- Service: See Catalog
- Description: 56-Way F MX123 Series, Sealed (BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: Terminal Repair Kit
- Release Tool/Test Probe: Terminal Repair Kit

#### Engine Control Module (ECM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 PU | 420 | Cruise Control Release Signal (K34)
3 | -- | -- | Not Used
4 | 0.35 D-GN/WH | 1559 | 4WD Low Signal (4WD)
5-6 | -- | -- | Not Used
7 | 0.8 L-BU | 20 | Stop Lamp Control
8 | -- | -- | Not Used
9 | 0.35 BK | 2759 | Low Reference
10-11 | -- | -- | Not Used
12 | 0.35 BN/WH | 419 | MIL Control
13 | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control
14 | -- | -- | Not Used
15 | 0.35 PU | 1807 | Class 2 Serial Data
16 | 0.35 PU | 1807 | Class 2 Serial Data
17 | -- | -- | Not Used
18 | 0.5 BN | 4 | Ignition Voltage
19 | 0.35 PK | 639 | Ignition Voltage
20 | 0.35 OG | 440 | Battery Positive Voltage
21-25 | -- | -- | Not Used
26 | 0.35 YE/BK | 625 | Starter Enable Relay Control
27-28 | -- | -- | Not Used
29 | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
30-32 | -- | -- | Not Used
33 | 0.35 WH/BK | 1164 | 5-Volt Reference
34 | 0.35 GY | 2709 | 5-Volt Reference
35 | 0.35 TN | 1274 | 5-Volt Reference
36 | 0.35 BN | 1271 | Low Reference
37 | 0.35 PU | 1272 | Low Reference
38-39 | -- | -- | Not Used
40 | 0.35 YE | 5991 | Powertrain Relay Control
41-43 | -- | -- | Not Used
44 | 0.35 PU | 1589 | Fuel Level Sensor Signal
45-46 | -- | -- | Not Used
47 | 0.35 D-BU | 1161 | APP Sensor 1 Signal
48 | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
49 | 0.35 L-BU | 1162 | APP Sensor 2 Signal
50 | -- | -- | Not Used
51 | 0.35 PU | 421 | AIR Solenoid Relay Control (K18)
52 | -- | -- | Not Used
53 | 0.35 D-GN/WH | 459 | A/C Compressor Clutch Relay Control
54 | -- | -- | Not Used
55 | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control
56 | -- | -- | Not Used

### Engine Control Module (ECM) X2

#### Connector Part Information

- OEM: 34566-7703
- Service: See Catalog
- Description: 73-Way F MX123 34566 Series (BK)

#### Terminal Part Information

- Pins: 1-9, 11-13, 16-19, 23, 24, 27, 29, 32-35, 39, 40, 42-44, 48, 49, 52-55, 59, 60, 62-64, 66, 72
- Terminal/Tray: 33467-0005/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

- Pins: 73
- Terminal/Tray: 7116-4152-02/9
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Engine Control Module (ECM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 2121 | IC 1 Control
2 | 0.5 TN/WH | 1653 | HO2S Low Signal Sensor 1 (LLR/LLV)
0.5 TN | 1664 | HO2S Low Signal - Bank 1 Sensor 1 (LH8)
3 | 0.5 D-GN | 1655 | HO2S High Signal - Sensor 1 (LLR/LLV)
0.5 PU/WH | 1665 | HO2S High Signal - Bank 1 Sensor 1 (LH8)
4 | 0.5 PU/WH | 1668 | HO2S High Signal - Bank 1 Sensor 2 (LH8)
HO2S High Signal - Sensor 2 (LLR/LLV)
5 | 0.5 TN/WH | 1669 | HO2S Low Signal - Bank 1 Sensor 2 (LH8)
HO2S Low Signal - Sensor 2 (LLR/LLV)
6 | 0.8 L-BU | 1876 | Knock Sensor 2 Signal (LH8)
7 | 0.8 GY | 2303 | Knock Sensor 2 Signal (LH8)
8 | 0.8 D-BU | 496 | Knock Sensor 1 Signal (LH8)
0.35 L-BU | 1876 | Knock Sensor Signal (LLR/LLV)
9 | 0.8 GY | 1716 | Knock Sensor 1 Signal (LH8)
0.35 GY | 2303 | Knock Sensor Signal (LLR/LLV)
10 | -- | -- | Not Used
11 | 0.5 YE | 581 | TAC Motor Control - 1
12 | 0.5 BN | 582 | TAC Motor Control - 2
13 | 0.5 PK | 739 | Ignition Voltage
14 | 0.5 BN | 2198 | CMP Actuator Solenoid Control (LLR/LLV)
15 | -- | -- | Not Used
16 | 0.8 PK/BK | 1746 | Fuel Injector 3 Control (LH8)
17 | 0.5 PU/WH | 2128 | IC 8 Control (LH8)
0.5 L-BU | 2123 | IC 3 Control (LLR/LLV)
18 | 0.5 D-GN/WH | 2124 | IC 4 Control (LH8)
19 | 0.5 BN/WH | 2130 | Low Reference (LH8)
20-22 | -- | -- | Not Used
23 | 0.5 OG | 6260 | Low Reference (LH8)
0.5 PK/BK | 632 | Low Reference (LLR/LLV)
24 | 0.5 BK | 2755 | Low Reference
25-26 | -- | -- | Not Used
27 | 0.5 GY/BK | 6272 | Low Reference (LH8)
0.5 D-BU/WH | 1869 | Low Reference (LLR/LLV)
28 | -- | -- | Not Used
29 | 0.5 BK | 2752 | Low Reference
30-31 | -- | -- | Not Used
32 | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control (LH8))
0.5 L-BU/BK | 844 | Fuel Injector 4 Control (LLR/LLV)
33 | 0.5 RD | 2127 | IC 7 Control (LH8)
0.5 D-GN/WH | 2124 | IC 4 Control (LLV)
0.5 D-GN | 2125 | IC 5 Control (LLR)
34 | 0.5 D-GN | 2125 | IC 5 Control (LH8)
35 | 0.5 BN | 2129 | Low Reference (LH8)
36-38 | -- | -- | Not Used
39 | 0.5 D-BU | 6259 | 5-Volt Reference 1 (LH8)
0.35 RD | 631 | 5-Volt Reference (LLR/LLV)
40 | 0.5 GY | 2705 | 5-Volt Reference 1 (LH8)
41 | -- | -- | Not Used
42 | 0.5 BK | 2760 | Low Reference
43 | 0.5 PU/WH | 6270 | 5-Volt Reference (LH8)
0.5 L-GN | 1867 | 5-Volt Reference (LLR/LLV)
44 | 0.5 GY | 2701 | 5-Volt Reference
45 | -- | -- | Not Used
46 | 0.35 BK | 2199 | Low Reference (LLR/LLV)
47 | -- | -- | Not Used
48 | 0.8 D-BU/WH | 878 | Fuel Injector 8 Control (LH8)
0.5 PK/BK | 1746 | Fuel Injector 3 Control (LLR/LLV)
49 | 0.8 BK/WH | 845 | Fuel Injector 5 Control (LH8)
50-51 | -- | -- | Not Used
52 | 0.8 YE/BK | 846 | Fuel Injector 6 Control (LH8)
0.5 L-GN/BK | 1745 | Fuel Injector 2 Control (LLR)
53 | 0.5 RD/WH | 2122 | IC 2 Control (LH8)
0.5 OG/WH | 2122 | IC 2 Control (LLV/)
0.5 D-GN/WH | 2124 | IC 4 Control (LLR)
54 | 0.5 L-BU/WH | 2126 | IC 6 Control (LH8)
0.5 RD/WH | 2122 | IC 2 Control (LLR)
55 | 0.5 L-BU | 2123 | IC 3 Control (LH8)
56-58 | -- | -- | Not Used
59 | 0.5 D-BU/WH | 6265 | CMP Sensor Signal (LH8)
0.5 BK | 630 | Low Reference (LLR/LLV)
60 | 0.5 TN/WH | 331 | Oil Pressure Sensor Signal (LH8)
61 | -- | -- | Not Used
62 | 0.5 L-BU | 6289 | IAT Sensor Signal
63 | 0.5 WH/BK | 6271 | CKP Sensor Signal (LH8)
0.5 YE/BK | 1868 | CKP Sensor Signal
64 | 0.5 D-GN | 485 | TP Sensor 1 Signal
65 | -- | -- | Not Used
66 | 0.5 PU | 486 | TP Sensor 2 Signal
67 | 0.5 YE | 492 | MAF Sensor Signal
68 | 0.5 BK/WH | 3113 | HO2S Heater Low Control - Bank 1 Sensor 1 (LH8)
0.5 D-GN | 676 | HO2S Heater High Control - Sensor 1 (LLV/LLR)
69 | 0.5 BK/WH | 3122 | HO2S Heater Low Control - Bank 1 Sensor 2 (LH8)
0.5 BK/WH | 1423 | HO2S Heater Low Control - Sensor 2 (LLR/LLV)
70 | 0.8 L-BU/BK | 844 | Fuel Injector 4 Control (LH8)
71 | 0.8 RD/BK | 877 | Fuel Injector 7 Control (LH8)
0.5 L-BU/BK | 844 | Fuel Injector 4 Control (LLV)
0.5 BK/WH | 845 | Fuel Injector 5 Control (LLR)
72 | 0.5 BK | 1744 | Fuel Injector 1 Control
73 | 2 BK/WH | 451 | Ground

### Engine Control Module (ECM) X3

#### Connector Part Information

- OEM: 34566-1243
- Service: See Catalog
- Description: 73-Way F MX123 34566 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 33467-0005/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 TN | 1667 | HO2S Low Signal - Bank 2 Sensor 1 (LH8)
4 | 0.5 PU | 1666 | HO2S High Signal - Bank 2 Sensor 1 (LH8)
5 | 0.5 PU | 1670 | HO2S High Signal - Bank 2 Sensor 2 (LH8)
6 | 0.5 TN | 1671 | HO2S Low Signal - Bank 2 Sensor 2 (LH8)
7 | 0.5 PU | 5428 | Generator Regulator Control
8 | -- | -- | Not Used
9 | 0.5 BN | 436 | AIR Relay Control (K18)
10-11 | -- | -- | Not Used
12 | 0.35 TN/BK | 464 | Delivered Torque Signal
13-14 | -- | -- | Not Used
15 | 0.5 L-GN | 3212 | HO2S Heater Low Control - Bank 2 Sensor 1 (LH8)
16 | -- | -- | Not Used
17 | 0.35 OG/BK | 463 | Requested Torque Signal
18-20 | -- | -- | Not Used
21 | 0.5 BK/WH | 2751 | Low Reference
22 | -- | -- | Not Used
23 | 0.5 OG/BK | 469 | Low Reference
24-25 | -- | -- | Not Used
26 | 0.5 D-BU/WH | 6785 | Low Reference (K18)
27 | 0.5 D-GN/WH | 6294 | Low Reference (MA5)
28 | -- | -- | Not Used
29 | 0.5 GY | 23 | Generator Field Duty Cycle Signal
30-32 | -- | -- | Not Used
33 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus -
34 | -- | -- | Not Used
35 | 0.5 TN | 2761 | Low Reference
36 | -- | -- | Not Used
37 | 0.5 GY | 2700 | 5-Volt Reference
38 | -- | -- | Not Used
39 | 0.5 GY | 2704 | 5-Volt Reference
40-41 | -- | -- | Not Used
42 | 0.5 BN/WH | 6789 | 5-Volt Reference (K18)
43 | 0.5 D-GN | 6293 | 5-Volt Reference (MA5)
44-45 | -- | -- | Not Used
46 | 0.35 OG/BK | 1786 | Park/Neutral Signal
47 | -- | -- | Not Used
48 | 0.5 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
49 | -- | -- | Not Used
50 | 0.5 RD/WH | 3223 | HO2S Heater Low Control - Bank 2 Sensor 2 (LH8)
51-52 | -- | -- | Not Used
53 | 0.5 TN/WH | 2500 | High Speed GMLAN Serial Data Bus +
54 | -- | -- | Not Used
55 | 0.5 YE | 410 | ECT Sensor Signal
56 | -- | -- | Not Used
57 | 0.5 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
58 | -- | -- | Not Used
59 | 0.5 L-GN | 432 | MAP Sensor Signal
60-61 | -- | -- | Not Used
62 | 0.5 YE | 6787 | Air Injection Reaction Control Valve Control (K18)
63 | 0.5 D-BU | 6306 | Clutch Pedal Position Signal (MA5)
64 | -- | -- | Not Used
65 | 0.35 TN/BK | 231 | Oil Pressure Switch Signal (LLR/LLV)
66 | 0.5 PU/WH | 821 | VSS High Signal (MA5)
67 | 0.5 L-GN/BK | 822 | VSS Low Signal (MA5)
68-73 | -- | -- | Not Used

### Engine Coolant Temperature (ECT) Sensor (LH8)

#### Connector Part Information

- OEM: 15449028
- Service: 88987993
- Description: 2-Way F 150 GT Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Engine Coolant Temperature (ECT) Sensor (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 410 | ECT Sensor Signal
B | 0.35 BK | 2761 | Low Reference

### Engine Coolant Temperature (ECT) Sensor (LLR/LLV)

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Engine Coolant Temperature (ECT) Sensor (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 2761 | Low Reference
B | 0.35 YE | 410 | ECT Sensor Signal

### Engine Oil Pressure (EOP) Sensor (LH8)

#### Connector Part Information

- OEM: 13589761
- Service: 12126436
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Engine Oil Pressure (EOP) Sensor (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/WH | 331 | Oil Pressure Sensor Signal
2 | 0.5 GY | 2705 | 5-Volt Reference
3 | 0.5 BK | 2755 | Low Reference

### Engine Oil Pressure (EOP) Switch (LLR/LLV)

#### Connector Part Information

- OEM: 12065400
- Service: 12126436
- Description: 4-Way F Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Engine Oil Pressure (EOP) Switch (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/BK | 231 | Oil Pressure Switch Signal
B | 0.5 BK | 2755 | Low Reference
C-D | -- | -- | Not Used

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.35 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 1640 | Battery Positive Voltage
B | 0.35 WH | 1310 | EVAP Canister Vent Solenoid Control

### Evaporator Temperature Sensor (C60)

#### Connector Part Information

- OEM: 15368694
- Service: 88953272
- Description: 3-Way F Metri-Pack 150 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 173630-7/7
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-33 (YE)

#### Evaporator Temperature Sensor (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 66 | A/C Request Signal
2 | 0.35 D-GN/WH | 762 | A/C Request Signal
3 | 0.35 BK | 2050 | Ground

### Fog Lamp - Left Front (T96)

#### Connector Part Information

- OEM: 12059183
- Service: 12101898
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Left Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Fog Lamps Control
B | 0.5 BK | 850 | Ground

### Fog Lamp - Right Front (T96)

#### Connector Part Information

- OEM: 12059183
- Service: 12101898
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Right Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Fog Lamps Control
B | 0.5 BK | 850 | Ground

### Front Drive Axle Actuator (4WD)

#### Connector Part Information

- OEM: 12077591
- Service: 12117277
- Description: 5-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Front Drive Axle Actuator (4WD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK/WH | 1695 | Axle Switch Signal
B | 0.35 L-BU | 1296 | Axle Actuator - Control
C | 0.5 PK | 1539 | Ignition Voltage
D | -- | -- | Not Used
E | 0.5 BK | 550 | Ground

### Fuel Injector 1 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 1 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 539 | Ignition Voltage
B | 0.5 BK | 1744 | Fuel Injector 1 Control

### Fuel Injector 1 (LLV)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 1 (LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 839 | Ignition Voltage
B | 0.5 BK | 1744 | Fuel Injector 1 Control

### Fuel Injector 1 (LLR)

#### Connector Part Information

- OEM: 15411634
- Service: See Catalog
- Description: 2-Way F Micro-Pack 064 Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 15305174/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Fuel Injector 1 (LLR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 BK | 1744 | Fuel Injector 1 Control

### Fuel Injector 2 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 2 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control

### Fuel Injector 2 (LLV)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 2 (LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 839 | Ignition Voltage
B | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control

### Fuel Injector 2 (LLR)

#### Connector Part Information

- OEM: 15411634
- Service: See Catalog
- Description: 2-Way F Micro-Pack 064 Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 15305174/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Fuel Injector 2 (LLR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control

### Fuel Injector 3 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 3 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 539 | Ignition Voltage
B | 0.5 PK/BK | 1746 | Fuel Injector 3 Control

### Fuel Injector 3 (LLV)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 3 (LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 839 | Ignition Voltage
B | 0.5 PK/BK | 1746 | Fuel Injector 3 Control

### Fuel Injector 3 (LLR)

#### Connector Part Information

- OEM: 15411634
- Service: See Catalog
- Description: 2-Way F Micro-Pack 064 Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 15305174/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Fuel Injector 3 (LLR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 PK/BK | 1746 | Fuel Injector 3 Control

### Fuel Injector 4 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 4 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 L-BU/BK | 1745 | Fuel Injector 4 Control

### Fuel Injector 4 (LLV)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 4 (LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 839 | Ignition Voltage
B | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Injector 4 (LLR)

#### Connector Part Information

- OEM: 15411634
- Service: See Catalog
- Description: 2-Way F Micro-Pack 064 Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 15305174/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Fuel Injector 4 (LLR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Injector 5 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 5 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 539 | Ignition Voltage
B | 0.5 BK/WH | 845 | Fuel Injector 5 Control

### Fuel Injector 5 (LLR)

#### Connector Part Information

- OEM: 15411634
- Service: See Catalog
- Description: 2-Way F Micro-Pack 064 Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 15305174/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Fuel Injector 5 (LLR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 BK/WH | 845 | Fuel Injector 5 Control

### Fuel Injector 6 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 6 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 YE/BK | 846 | Fuel Injector 6 Control

### Fuel Injector 7 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 7 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 539 | Ignition Voltage
B | 0.5 RD/BK | 877 | Fuel Injector 7 Control

### Fuel Injector 8 (LH8)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Injector 8 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 439 | Ignition Voltage
B | 0.5 D-BU/WH | 878 | Fuel Injector 8 Control

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 13521459
- Service: 19152589
- Description: 4-Way F GT 280 Series Sealed 5.8 (BK)

#### Terminal Part Information

- Pins: A, D
- Terminal/Tray: 15304720/19
- Core/Insulation Crimp: 4/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: C, D
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Fuel Pump and Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 PK | 1580 | Low Reference
B | 0.35 PU | 1589 | Fuel Level Sensor Signal - Primary
C | 0.35 BK | 2759 | Low Reference
D | 2 GY | 120 | Fuel Pump Control

### Fuel Pump Flow Control Module

#### Connector Part Information

- OEM: 13570966
- Service: See Catalog
- Description: 47-Way F ASG Series Sealed (BK)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 12129497/1
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 5, 10, 15, 17, 36
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins 5, 10, 36 - E/1
- Core/Insulation Crimp: Pins 15, 17 - E/5
- Release Tool/Test Probe: 15315247/J-35616-2A (PU)

- Pins: 6, 7
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 16
- Terminal/Tray: 15304720/19
- Core/Insulation Crimp: 4/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 32
- Terminal/Tray: 12077413/4
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 44
- Terminal/Tray: 05297428/4
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fuel Pump Flow Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 BK | 850 | Ground
2-4 | -- | -- | Not Used
5 | 0.5 GY | 7447 | Low Reference
6 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
7 | 0.5 TN/WH | 2500 | High Speed GMLAN Serial Data Bus (+)
8-9 | -- | -- | Not Used
10 | 0.5 PU | 7446 | Fuel Line Pressure Sensor Signal
11-12 | -- | -- | Not Used
13 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control - Primary
14 | -- | -- | Not Used
15 | 0.5 PK | 439 | Ignition Voltage
16 | 2 PK | 1580 | Low Reference
17 | 0.5 BN | 4 | Ignition Voltage
18-20 | -- | -- | Not Used
21 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
22 | 0.5 TN/WH | 2500 | High Speed GMLAN Serial Data Bus (+)
23-31 | -- | -- | Not Used
32 | 3 OR | 1940 | Battery Positive Voltage
33-35 | -- | -- | Not Used
36 | 0.5 BN | 7445 | 5-Volt Reference
37-43 | -- | -- | Not Used
44 | 0.5 GY | 7443 | Fuel System Control Module Shield Extension
45-46 | -- | -- | Not Used
47 | 2 GY | 120 | Fuel Pump Supply Voltage

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 13522407
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
2 | 0.35 BK | 2759 | Low Reference
3 | 0.35 GY | 2709 | 5-Volt Reference

### Generator X1

#### Connector Part Information

- OEM: 12186308
- Service: 89046837
- Description: 2-Way F Timer Junior Power Timer Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 647/J-35616-4A (PU)

#### Generator X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 RD | 225 | Generator Turn On Signal
2 | 0.5 GY | 23 | Generator Field Duty Cycle Signal

### Generator Battery Control Module

#### Connector Part Information

- OEM: 15326842
- Service: 15326842
- Description: 10-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, B, D, F, J, K
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 647/J-35616-4A (PU)

- Pins: C, H
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: 2/1
- Release Tool/Test Probe: 647/J-35616-4A (PU)

#### Generator Battery Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 2040 | Battery Positive Voltage
B | 0.5 GY | 23 | Generator Field Duty Cycle Signal
C | 1 OG | 2040 | Battery Positive Voltage
D | 0.5 RD | 225 | Generator Turn On Signal
E | -- | -- | Not Used
F | 0.5 BK/WH | 451 | Ground
G | -- | -- | Not Used
H | 1 BK/WH | 451 | Ground
J | 0.35 PU | 5428 | Generator Regulator Control
K | 0.35 PU | 1807 | Class 2 Serial Data

### Hazard Warning Switch

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Hazard Warning Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 8 | Instrument Panel Lamps Dimmer Switch Signal
B | 0.35 BK | 2050 | Ground
C | 0.35 WH | 111 | Hazard Switch Signal

### Headlamp - Left High Beam (TT5)

#### Connector Part Information

- OEM: 12059183
- Service: 12101898
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Headlamp - Left High Beam (TT5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 640 | Headlamp Control
B | 0.35 PK | 1200 | High Beam Switched Ground

### Headlamp - Right High Beam (TT5)

#### Connector Part Information

- OEM: 12059183
- Service: 12101898
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Headlamp - Right High Beam (TT5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 640 | Headlamp Control
B | 0.35 PK | 1200 | High Beam Switched Ground

### Headlamp - Left (without TT5)

#### Connector Part Information

- OEM: 12034372
- Service: 12117369
- Description: 3-Way F Metri-Pack 800 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12020634/18
- Core/Insulation Crimp: Pins A, C - 4/B
- Core/Insulation Crimp: Pins B - See Terminal Repair Kit
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

#### Headlamp - Left (without TT5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 OG | 640 | Headlamp Control
B | 1 PK | 1200 | High Beam Switched Ground
C | 1 D-BU | 1201 | Low Beam Switched Ground

### Headlamp - Left Low Beam (TT5)

#### Connector Part Information

- OEM: 12059181
- Service: 12101897
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Headlamp - Left Low Beam (TT5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 640 | Headlamp Control
B | 0.35 D-BU | 1201 | Low Beam Switched Ground

### Headlamp - Right Low Beam (TT5)

#### Connector Part Information

- OEM: 12059181
- Service: 12101897
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Headlamp - Right Low Beam (TT5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 OG | 640 | Headlamp Control
B | 1 D-BU | 1201 | Low Beam Switched Ground

### Headlamp - Right (without TT5)

#### Connector Part Information

- OEM: 12034372
- Service: 12117369
- Description: 3-Way F Metri-Pack 800 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12020634/18
- Core/Insulation Crimp: Pins A, C - 4/B
- Core/Insulation Crimp: Pins B - See Terminal Repair Kit
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

#### Headlamp - Right (without TT5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 OG | 640 | Headlamp Control
B | 1 PK | 1200 | High Beam Switched Ground
C | 1 D-BU | 1201 | Low Beam Switched Ground

### Headlamp and Panel Dimmer Switch

#### Connector Part Information

- OEM: 15405512
- Service: 88986257
- Description: 14-Way F 035 ILAG5 (GN)

#### Terminal Part Information

- Terminal/Tray: IL-AG5-C1-5000 /20
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: J-38125-211/J-35616-64B (L-BU)

#### Headlamp and Panel Dimmer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU/WH | 1495 | Dome Override Switch Signal
2 | 0.35 BN/WH | 301 | Park Lamp Relay Control
3 | 0.35 PU | 719 | Low Reference
4 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
5 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
6 | 0.35 GY | 8 | Instrument Panel Lamps Dimmer Switch Signal
7 | 0.35 OG | 192 | Fog Lamps Enable (T96)
8 | 0.35 YE | 183 | Front Fog Lamp Indicator Control
9 | -- | -- | Not Used
10 | 0.35 WH/BK | 158 | Cargo Lamp Switch Signal (TR9)
11 | 0.35 PU | 328 | Interior Lamp Switch Signal
12-13 | -- | -- | Not Used
14 | 0.35 BN/WH | 230 | Instrument Panel Lamps Dimming Control

### Heated Oxygen Sensor (HO2S) 1 (LLR/LLV)

#### Connector Part Information

- OEM: 12146046
- Service: 15306365
- Description: 4-Way F Metri-Pack 150 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Oxygen Sensor (HO2S) 1 (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 1653 | HO2S Low Signal
B | 0.5 D-GN | 1655 | HO2S High Signal
C | -- | -- | Not Available
D | 0.5 PK | 414 | HO2S - Heater Elements - Control
E | 0.5 D-GN | 676 | HO2S Heater High Control

### Heated Oxygen Sensor (HO2S) 2 (LLR/LLV)

#### Connector Part Information

- OEM: 12092840
- Service: 15306311
- Description: 4-Way M Metri-Pack 150 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) 2 (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 1669 | HO2S Low Signal
B | 0.5 PU/WH | 1668 | HO2S High Signal
C | -- | -- | Not Used
D | 0.5 PK | 414 | HO2S - Heater Elements - Control
E | 0.5 BK/WH | 1423 | HO2S Heater Low Control

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LH8)

#### Connector Part Information

- OEM: 12160825
- Service: 15305801
- Description: 4-Way M Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 1664 | HO2S Low Signal - Bank 1 Sensor 1
B | 0.5 PU/WH | 1665 | HO2S High Signal - Bank 1 Sensor 1
C | -- | 3113 | HO2S Heater Low Control - Bank 1 Sensor 1
D | 0.5 PK | 414 | Ignition Voltage

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LH8)

#### Connector Part Information

- OEM: 12092839
- Service: 12092839
- Description: 4-Way M Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 1669 | HO2S Low Signal - Bank 1 Sensor 2
B | 0.5 PU/WH | 1668 | HO2S High Signal - Bank 1 Sensor 2
C | -- | -- | Not Available
D | 0.5 PK | 414 | Ignition Voltage
E | 0.5 BK/WH | 3122 | HO2S Heater Low Control - Bank 1 Sensor 2

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LH8)

#### Connector Part Information

- OEM: 12160825
- Service: 15305801
- Description: 4-Way M Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 1667 | HO2S Low Signal - Bank 2 Sensor 1
B | 0.5 PU | 1666 | HO2S High Signal - Bank 2 Sensor 1
C | 0.5 L-GN | 3212 | HO2S Heater Low Control - Bank 2 Sensor 1
D | 0.5 PK | 414 | Ignition Voltage

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LH8)

#### Connector Part Information

- OEM: 12092839
- Service: 12092839
- Description: 4-Way M Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 1671 | HO2S Low Signal - Bank 2 Sensor 2
B | 0.5 PU | 1670 | HO2S High Signal - Bank 2 Sensor 2
C | -- | -- | Not Available
D | 0.5 PK | 414 | Ignition Voltage
E | 0.5 RD/WH | 3223 | HO2S Heater Low Control - Bank 2 Sensor 2

### Heated Seat Element - Driver Back (KA1)

#### Connector Part Information

- OEM: 12059254
- Service: 12126020
- Description: 2-Way M Metri-Pack 150 Series (L-GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Driver Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | -- | Ground
B | YE | -- | Heated Seat Back Element Control

### Heated Seat Element - Passenger Back (KA1)

#### Connector Part Information

- OEM: 12059254
- Service: 12126020
- Description: 2-Way M Metri-Pack 150 Series (L-GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Passenger Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | -- | Ground
B | YE | -- | Heated Seat Back Element Control

### Horn Assembly

#### Connector Part Information

- OEM: 15421930
- Service: 89046631
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12176636/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Horn Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 850 | Ground
B | 0.35 D-GN | 29 | Horn Control

### Horn Switch

#### Connector Part Information

- OEM: 12092133
- Service: 12167133
- Description: 1-Way F Metri-Pack 630 Series Self Locking (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Horn Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN | 28 | Horn Relay Control

### HVAC Control Module X1

#### Connector Part Information

- OEM: 12064980
- Service: 12102629
- Description: 9-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### HVAC Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
7 | 0.35 D-GN | 71 | OFF Blower Motor Control (C60)
8 | 0.35 BN | 141 | Ignition Voltage
9 | 0.35 L-GN | 66 | A/C Request Signal (C60)
10 | 0.35 L-GN/BK | 1647 | Recirculation Door Control B (C60)
11 | 0.35 PK/WH | 1648 | Recirculation Door Control A (C60)
12 | 0.35 PK | 2216 | A/C Recirculation Request Signal
13 | 0.35 GY | 8 | Instrument Panel Lamps Dimmer Switch Signal
14 | 0.35 BK | 2050 | Ground
15 | -- | -- | Not Used

### HVAC Control Module X2

#### Connector Part Information

- OEM: 12064998
- Service: 15306189
- Description: 8-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: B, E, F, G, H
- Terminal/Tray: 12015858/4
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### HVAC Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 71 | OFF Blower Motor Control (C60)
B | 2 BK | 2050 | Ground
C-D | -- | -- | Not Used
E | 2 OG | 52 | Blower Motor High Control
F | 2 L-BU | 72 | Medium 2 Blower Motor Control
G | 2 TN | 63 | Blower Motor Medium 1 Control
H | 2 YE | 60 | Blower Motor Low Control

### I/P Courtesy Lamp - Left

#### Connector Part Information

- OEM: 15437400
- Service: See Catalog
- Description: 2-Way F LP SOC Wedge (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### I/P Courtesy Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 1732 | Courtesy Lamps Control
B | 0.35 WH | 156 | Courtesy Lamp Low Control

### I/P Courtesy Lamp - Right

#### Connector Part Information

- OEM: 15437400
- Service: See Catalog
- Description: 2-Way F LP SOC Wedge (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### I/P Courtesy Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 1732 | Courtesy Lamps Control
B | 0.35 WH | 156 | Courtesy Lamp Low Control

### Ignition Coil 1 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 1 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 550 | Ignition Voltage
B | 0.35 PU | 2129 | IC 1 Control
C | 0.5 BK | 2121 | Ground
D | 0.8 PK | 239 | Ignition Voltage

### Ignition Coil 1 (LLR/LLV)

#### Connector Part Information

- OEM: 15355370
- Service: 15306431
- Description: 3-Way F GT 150 Series Sealed 3.2x4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 1 (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 239 | Ignition Voltage
B | 0.35 PU | 2121 | IC 1 Control
C | 0.5 BK | 550 | Ground

### Ignition Coil 2 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 2 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 550 | Ground
B | 0.5 BN | 2130 | Low Reference
C | 0.5 RD | 2122 | IC 2 Control
D | 0.8 PK | 839 | Ignition Voltage

### Ignition Coil 2 (LLR/LLV)

#### Connector Part Information

- OEM: 15355370
- Service: 15306431
- Description: 3-Way F GT 150 Series Sealed 3.2x4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 2 (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 239 | Ignition Voltage
B | 0.35 RD/WH | 2122 | IC 2 Control
C | 0.5 BK | 550 | Ground

### Ignition Coil 3 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 3 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 550 | Ground
B | 0.5 BN | 2129 | Low Reference
C | 0.5 L-BU | 2123 | IC 2 Control
D | 0.8 PK | 239 | Ignition Voltage

### Ignition Coil 3 (LLR/LLV)

#### Connector Part Information

- OEM: 15355370
- Service: 15306431
- Description: 3-Way F GT 150 Series Sealed 3.2x4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 3 (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 239 | Ignition Voltage
B | 0.35 L-BU | 2123 | IC 3 Control
C | 0.5 BK | 550 | Ground

### Ignition Coil 4 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 4 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 550 | Ground
B | 0.5 BN | 2130 | Low Reference
C | 0.5 D-GN | 2124 | IC 4 Control
D | 0.8 PK | 839 | Ignition Voltage

### Ignition Coil 4 (LLR/LLV)

#### Connector Part Information

- OEM: 15355370
- Service: 15306431
- Description: 3-Way F GT 150 Series Sealed 3.2x4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 4 (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 239 | Ignition Voltage
B | 0.35 D-GN/WH | 2124 | IC 4 Control
C | 0.5 BK | 550 | Ground

### Ignition Coil 5 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 5 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 550 | Ground
B | 0.5 BN | 2129 | Low Reference
C | 0.5 D-GN | 2125 | IC 5 Control
D | 0.8 PK | 239 | Ignition Voltage

### Ignition Coil 5 (LLR)

#### Connector Part Information

- OEM: 15355370
- Service: 15306431
- Description: 3-Way F GT 150 Series Sealed 3.2x4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 5 (LLR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 239 | Ignition Voltage
B | 0.35 D-GN | 2125 | IC 5 Control
C | 0.5 BK | 550 | Ground

### Ignition Coil 6 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 6 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 550 | Ground
B | 0.5 BN | 2130 | Low Reference
C | 0.5 L-BU | 2126 | IC 5 Control
D | 0.8 PK | 839 | Ignition Voltage

### Ignition Coil 7 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 7 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 550 | Ground
B | 0.5 BN | 2129 | Low Reference
C | 0.5 RD | 2127 | IC 5 Control
D | 0.8 PK | 239 | Ignition Voltage

### Ignition Coil 8 (LH8)

#### Connector Part Information

- OEM: 15439568
- Service: 88987184
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A, D: E/1
- Core/Insulation Crimp: Pins B, C: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 8 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 550 | Ground
B | 0.5 BN | 2130 | Low Reference
C | 0.5 D-GN | 2128 | IC 8 Control
D | 0.8 PK | 839 | Ignition Voltage

### Ignition Switch

#### Connector Part Information

- OEM: IL-AG5-6S-S3C1
- Service: 88987854
- Description: 6-Way F (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH/RD | 4 | Ignition Voltage
2 | 0.5 WH/BK | 1740 | Battery Positive Voltage
3 | 0.5 WH/GN | 338 | Ignition Voltage
4 | 0.5 WH/BU | 1390 | Ignition Voltage
5 | 0.5 WH/YE | 1073 | Ignition Key Resistor Signal
6 | -- | -- | Not Used

### Inflatable Restraint Front End Sensor - Left

#### Connector Part Information

- OEM: 15356724
- Service: 15306418
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 354 | Discriminating Sensor - Signal
B | 0.35 GY | 349 | Discriminating Sensor - Left - Signal

### Inflatable Restraint Front End Sensor - Right

#### Connector Part Information

- OEM: 15356724
- Service: 15306418
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal
B | 0.35 YE | 1834 | Front End Sensor - Voltage

### Inflatable Restraint I/P Module

#### Connector Part Information

- OEM: 15383139
- Service: Not Serviced
- Description: 4-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint I/P Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 3026 | I/P Module - Stage 2 - Low Control
2 | 0.5 GY | 3027 | I/P Module - Stage 2 - High Control
3 | 0.5 OG | 3024 | I/P Module - Stage 1 - Low Control
4 | 0.5 YE | 3025 | I/P Module - Stage 1 - High Control

### Inflatable Restraint Passenger Presence System (PPS) Module

#### Connector Part Information

- OEM: 15431682
- Service: See Catalog
- Description: 18-Way F Micro-Pack 100W Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Passenger Presence System (PPS) Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU | 2307 | Passenger Air Bag On Indicator Control
2 | 0.35 D-GN | 2308 | Passenger Air Bag Off Indicator Control
3 | -- | -- | Not Used
4 | 0.35 PU | 5611 | Passenger Seat Belt Tension Sensor Signal
5 | 0.35 BK/WH | 2151 | Ground
6 | 0.35 WH | 5608 | Occupant Pressure Sensor Signal
7 | 0.35 L-GN | 5609 | Occupant Pressure Sensor Voltage Reference
8 | -- | -- | Not Used
9 | 0.35 YE | 1139 | Ignition Voltage
10-13 | -- | -- | Not Used
14 | 0.35 TN | 5613 | Low Reference
15 | 0.35 GY | 5610 | Low Reference
16 | 0.35 L-BU | 5612 | 5-Volt Reference
17 | -- | -- | Not Used
18 | 0.35 PK | 2306 | Serial Data Link

### Inflatable Restraint Passenger Presence System (PPS) Sensor

#### Connector Part Information

- OEM: 15422250
- Service: 88987995
- Description: 3-Way F GT 150 Series (D-GY)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Passenger Presence System (PPS) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN | 5609 | Occupant Pressure Sensor Voltage Reference
B | 0.35 WH | 5608 | Occupant Pressure Sensor Signal
C | 0.35 GY | 5610 | Low Reference

### Inflatable Restraint Roof Rail Module - Left (ASF)

#### Connector Part Information

- OEM: 15383139
- Service: Not Serviced
- Description: 4-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Left (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 BN | 2137 | Side Impact Module - Left Front - High Control
4 | 0.5 YE/BK | 2138 | Side Impact Module - Left Front - Low Control

### Inflatable Restraint Roof Rail Module - Right (ASF)

#### Connector Part Information

- OEM: 15383139
- Service: Not Serviced
- Description: 4-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Right (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 BK/WH | 2135 | Side Impact Module - Right Front - High Control
4 | 0.5 L-GN | 2136 | Side Impact Module - Right Front - Low Control

### Inflatable Restraint Seat Position Sensor - Left

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Seat Position Sensor - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/WH | 2638 | Seat Position Sensor - Left - Signal
B | 0.35 BK/WH | 2644 | Low Reference

### Inflatable Restraint Seat Position Sensor - Right

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Seat Position Sensor - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/WH | 2645 | Seat Position Sensor - Right - Signal
B | 0.35 BK/WH | 2644 | Low Reference

### Inflatable Restraint Sensing and Diagnostic Module (SDM)

#### Connector Part Information

- OEM: 15449363
- Service: See Catalog
- Description: 42-Way F Micro-Pack 100 W (D-GY)

#### Terminal Part Information

- Pins: 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38
- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12122523/J-35616-6 (BN)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1139 | Ignition Voltage
2 | 0.35 TN/BK | 371 | Serial Data Link
3 | 0.35 BK/WT | 238 | Seat Belt Switch - Left
4 | 0.35 RD | 1362 | Seat Belt Switch - Right
5 | 0.35 GY | 349 | Discriminating Sensor - Left - Signal
6 | 0.35 YE | 1834 | Front End Sensor - Voltage
7 | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF)
8 | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage (ASF)
9 | 0.35 YE | 3025 | I/P Module - Stage 1 - High Control
10 | 0.35 OG | 3024 | I/P Module - Stage 1 - Low Control
11 | 0.35 BK | 407 | Low Reference
12 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
13 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
14 | 0.5 BK/WH | 2135 | Side Impact Module - Right Front - High Control (ASF)
15 | 0.5 L-GN | 2136 | Side Impact Module - Right Front - Low Control (ASF)
16 | 0.5 YE/BK | 2138 | Side Impact Module - Left Front - Low Control (ASF)
17 | 0.5 BN | 2137 | Side Impact Module - Left Front - High Control (ASF)
18-21 | -- | -- | Not Used
22 | 0.35 PU | 1807 | Class 2 Serial Data
23 | 0.35 PU | 1807 | Class 2 Serial Data
24 | 0.35 L-GN | 5055 | Seat Position Sensor - Left - Signal
25 | 0.35 L-BU | 5056 | Seat Position Sensor - Right - Signal
26 | 0.35 YE | 354 | Discriminating Sensor - Signal
27 | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal
28 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF)
29 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal (ASF)
30 | 0.5 GY | 3027 | I/P Module - Stage 2 - High Control
31 | 0.5 PU | 3026 | I/P Module - Stage 2 - Low Control
32 | 0.5 BK/WH | 2151 | Ground
33 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
34 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
35 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
36 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control
37 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
38 | 0.5 BK/WH | 2118 | Seat Belt Pretensioner - Left - High Control
39-42 | -- | -- | Not Used

### Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)

#### Connector Part Information

- OEM: 15356725
- Service: 88986455
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal
B | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage

### Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)

#### Connector Part Information

- OEM: 15356725
- Service: 88986455
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal
B | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage

### Inflatable Restraint Steering Wheel Module X1

#### Connector Part Information

- OEM: 54560208
- Service: See Catalog
- Description: 2-Way F ABX-3 Cord B (TN)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 3021 | Steering Wheel Module - Stage 1 - High Control
B | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control

### Inflatable Restraint Steering Wheel Module X2

#### Connector Part Information

- OEM: 54550271
- Service: See Catalog
- Description: 2-Way F ABX-3 Cord G (PK)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD | 3023 | Steering Wheel Module - Stage 2 - High Control
B | 0.5 WH | 3022 | Steering Wheel Module - Stage 2 - Low Control

### Inside Rearview Mirror (ISRVM)

#### Connector Part Information

- OEM:15441350
- Service: 15306351
- Description: 16-Way F 040 II (WH)

#### Terminal Part Information

- Terminal/Tray: 15445905/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12180559/J-35616-6 (BN)

#### Inside Rearview Mirror (ISRVM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
7 | 0.35 D-GN | 61 | Low Reference
8 | 0.35 BK | 850 | Ground
9 | 0.5 BN | 24 | Backup Lamp Control
10 | -- | -- | Not Used
11 | 0.35 D-BU | 2514 | Keypad Signal (UE1)
12 | 0.35 BK | 2515 | Keypad Control (UE1)
13 | 0.35 D-BU/WH | 339 | Ignition Voltage
14 | 0.35 GY | 2516 | Keypad Green LED Signal
15 | 0.35 BN/WH | 2517 | Keypad Red LED Signal (UE1)
16 | -- | -- | Not Used

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 10820547
- Service: 89046871
- Description: 18-Way F Quadlok Micro (BK)

#### Terminal Part Information

- Terminal/Tray: 928999-5/15
- Core/Insulation Crimp: Pins 1, 4, 5, 10, 11, 15, 16 - H/H
- Core/Insulation Crimp: Pins 6, 7 - J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Instrument Panel Cluster (IPC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG | 1440 | Battery Positive Voltage
2-3 | -- | -- | Not Used
4 | 0.35 BK/WH | 1151 | Ground
5 | 0.35 BN/WH | 419 | MIL Control
6 | 0.5 YE | 18 | Left Rear Turn Signal Lamps Control
7 | 0.5 D-GN | 19 | Right Rear Turn Signal Lamps Control
8-9 | -- | -- | Not Used
10 | 0.35 PU | 1807 | Class 2 Serial Data
11 | 0.35 PU | 1807 | Class 2 Serial Data
12-14 | -- | -- | Not Used
15 | 0.35 YE | 234 | Seat Belt Indicator Control
16 | 0.35 GY | 728 | Security Indicator Control
17-18 | -- | -- | Not Used

### Knock Sensor (KS) 1 (LH8)

#### Connector Part Information

- OEM: 15374222
- Service: 88953268
- Description: 2-Way F GT 150 Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: 2/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Knock Sensor (KS) 1 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-BU | 496 | KS 1 Signal
B | 0.8 GY | 1716 | KS 1 Signal

### Knock Sensor (KS) 2 (LH8)

#### Connector Part Information

- OEM: 15374222
- Service: 88953268
- Description: 2-Way F GT 150 Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Knock Sensor (KS) 2 (LH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 1876 | KS 2 Signal
B | 0.8 GY | 2303 | KS 2 Signal

### Knock Sensor (KS) (LLR/LLV)

#### Connector Part Information

- OEM: 15374222
- Service:15306631
- Description: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Knock Sensor (KS) (LLR/LLV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-BU | 1876 | KS Signal
B | 0.35 GY | 2303 | KS Signal

### License Lamp - Left

#### Connector Part Information

- OEM: 15300027
- Service: 12101855
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### License Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Control
B | 0.5 BK | 850 | Ground

### License Lamp - Right

#### Connector Part Information

- OEM: 15300027
- Service: 12101855
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### License Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Control
B | 0.5 BK | 850 | Ground

### Manifold Absolute Pressure (MAP) Sensor

#### Connector Part Information

- OEM: 15397338
- Service: See Catalog
- Description: 3-Way F 2.8 Timer Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-36/J-35616-35 (VT)

#### Manifold Absolute Pressure (MAP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 2704 | 5-Volt Reference
2 | 0.35 OG/BK | 469 | Low Reference
3 | 0.35 L-GN | 432 | MAP Sensor Signal

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: 15326822
- Service: 88987186
- Description: 5-Way F GT 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 492 | MAF Sensor Signal
B | 0.5 BK/WH | 451 | Ground
C | 0.5 PK | 439 | Ignition Voltage
D | 0.5 BK | 2760 | IAT Sensor Signal
E | 0.5 L-BU | 6289 | Low Reference

### Multifunction Switch - I/P

#### Connector Part Information

- OEM: 15332169
- Service: 88986447
- Description: 14-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Multifunction Switch - I/P

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 339 | Ignition Voltage
B | 0.35 L-GN/BK | 1563 | 2-HI Indicator - Control (4WD)
0.35 PU/WH | 1572 | TCS Requested Indicator Control (NW7)
C | 0.35 BN | 9 | Park Lamp Control
D | 0.35 TN/BK | 2308 | Passenger Air Bag Off Indicator Control
E | 0.35 PK | 2307 | Passenger Air Bag On Indicator Control
F | 0.35 BN | 1560 | Neutral Indicator Control (4WD)
G | 0.35 GY | 8 | Instrument Panel Lamp Dimmer Switch Signal
H | 0.35 BK | 2050 | Ground
0.5 BK | 2050 | Ground
J | 0.35 TN/BK | 1566 | 4-HI Indicator - Control (4WD)
0.35 BN/WH | 1571 | Traction Control Switch Signal (NW7)
K | -- | -- | Not Used
L | 0.35 YE | 234 | Seat Belt Indicator Control
M | 0.35 GY/BK | 1694 | 5-Volt Reference (4WD)
N | 0.35 L-BU/BK | 1693 | Switch Signal Low (4WD)
P | 0.35 PU/WH | 1565 | 4-LO Indicator - Control (4WD)

### Outside Rearview Mirror - Driver (DE6)

#### Connector Part Information

- OEM: 15383150
- Service: 89046644
- Description: 4-Way F 090 (WH)

#### Terminal Part Information

- Terminal/Tray: 15305180/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Outside Rearview Mirror - Driver (DE6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH | 81 | Driver Mirror Motor Right Control
2 | 0.35 L-GN | 1499 | Driver Mirror Motor Left/Down Control
3 | -- | -- | Not Used
4 | 0.35 YE | 88 | Driver Mirror Motor Up Control

### Outside Rearview Mirror - Passenger (DE6)

#### Connector Part Information

- OEM: 15383150
- Service: 89046644
- Description: 4-Way F 090 (WH)

#### Terminal Part Information

- Terminal/Tray: 15305180/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Outside Rearview Mirror - Passenger (DE6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 881 | Passenger Mirror Motor Right Control
2 | 0.35 L-BU/WH | 1497 | Passenger Mirror Motor Left/Down Control
3 | -- | -- | Not Used
4 | 0.35 BN/WH | 1498 | Passenger Mirror Motor Up Control

### Outside Rearview Mirror Switch (DE6)

#### Connector Part Information

- OEM: 15365903
- Service: 15365903
- Description: 10-Way F 050 050 (WH)

#### Terminal Part Information

- Terminal/Tray: 7116-1257-02/14
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 15315247/J-35616-12 (BU)

#### Outside Rearview Mirror Switch (DE6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU/WH | 1497 | Passenger Mirror Motor Left/Down Control
2 | 0.35 BN/WH | 1498 | Passenger Mirror Motor Up Control
3 | 0.35 YE | 88 | Driver Mirror Motor Up Control
4 | 0.35 OG | 1732 | Courtesy Lamps Control
5 | 0.35 BN | 9 | Park Lamp Control
6 | 0.35 BK | 850 | Ground
7 | 0.35 L-GN | 1499 | Driver Mirror Motor Left/Down Control
8 | 0.35 BK | 850 | Ground
9 | 0.35 WH | 81 | Driver Mirror Motor Right Control
10 | 0.35 RD/WH | 881 | Passenger Mirror Motor Right Control

### Park Brake Switch

#### Connector Part Information

- OEM: 8911256
- Service: 12102561
- Description: 1-Way F (WH)

#### Terminal Part Information

- Terminal/Tray: 12124515/1
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Park Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 1134 | Park Brake Switch Signal

### Park/Neutral Position (PNP) Switch (M30)

#### Connector Part Information

- OEM: 15416722
- Service: 88987526
- Description: Assembly Connector 12-Way F GT (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Park/Neutral Position (PNP) Switch (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 D-GN | 1433 | PNP/Clutch Start Switch Signal
4 | 0.35 YE | 772 | Transmission Range Switch Signal B
5 | 0.35 BK/WH | 771 | Transmission Range Switch Signal A
6 | 0.35 GY | 773 | Transmission Range Switch Signal C
7 | 0.5 BK/WH | 451 | Ground
8 | 0.35 WH | 776 | Transmission Range Switch Signal P
9 | -- | -- | Not Used
10 | 0.5 L-GN | 24 | Back-Up Lamp Control
11 | 0.5 PK | 539 | Ignition Voltage
12 | -- | -- | Not Used

### Park Lamp - Left Front

#### Connector Part Information

- OEM: 16530668
- Service: See Catalog
- Description: 3-Way F (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BN | -- | Park Lamp Control
G | BK | -- | Ground

### Park Lamp - Right Front

#### Connector Part Information

- OEM: 16530668
- Service: See Catalog
- Description: 3-Way F (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Park Lamp Control
B | BN | -- | Not Used
G | BK | -- | Ground

### Park/Turn Signal Lamp - Left

#### Connector Part Information

- OEM: 16530672
- Service: See Catalog
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | -- | Left Turn Signal Lamps Control
B | BN | -- | Park Lamp Control
BN | -- | Park Lamp Control
G | BK | -- | Ground
BK | -- | Ground

### Park/Turn Signal Lamp - Right

#### Connector Part Information

- OEM: 16530672
- Service: See Catalog
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | -- | Right Turn Signal Lamps Control
B | BN | -- | Park Lamp Control
BN | -- | Park Lamp Control
G | BK | -- | Ground
BK | -- | Ground

### Pressure Control (PC) Solenoid Valve (M30)

#### Connector Part Information

- OEM: 12146800
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 Series Delphi (L-GY)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Pressure Control (PC) Solenoid Valve (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 1228 | PC Solenoid Valve High Control
B | 0.5 L-BU | 1229 | PC Solenoid Valve Low Control

### Radio X1

#### Connector Part Information

- OEM: 12110088
- Service: 15306210
- Description: 24-Way F Micro-Pack 100 Series (GY)

#### Terminal Part Information

- Pins: A1, A2, A8, A9, A10, A11, B8, B9, B10, B11
- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

- Pins: A12, B1
- Terminal/Tray: 12146448/19
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Radio X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.35 PU | 1807 | Class 2 Serial Data
A2 | 0.35 PU | 1807 | Class 2 Serial Data
A3-A7 | -- | -- | Not Used
A8 | 0.5 GY | 118 | Left Front Speaker Output (-)
A9 | 0.5 TN | 201 | Left Front Speaker Output (+)
A10 | 0.5 D-BU | 46 | Right Rear Speaker Output (+)
A11 | 0.5 L-BU | 115 | Right Rear Speaker Output (-)
A12 | 1 BK/WH | 1151 | Ground
B1 | 1 OG | 1140 | Battery Positive Voltage
B2-B7 | -- | -- | Not Used
B8 | 0.5 YE | 116 | Left Rear Speaker Output (-)
B9 | 0.5 BN | 199 | Left Rear Speaker Output (+)
B10 | 0.5 L-GN | 200 | Right Front Speaker Output (+)
B11 | 0.5 D-GN | 117 | Right Front Speaker Output (-)
B12 | -- | -- | Not Used

### Radio X2

#### Connector Part Information

- OEM: 12064799
- Service: 15305996
- Description: 12-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Radio X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 BARE | 1573 | Drain Wire (U2K)
D-F | -- | -- | Not Used
G | 0.35 PU | 1807 | Class 2 Serial Data
H | 0.35 D-GN/WH | 368 | Remote Playback Device Right Audio Signal (U2K)
J | 0.35 BN/WH | 367 | Remote Playback Device Left Audio Signal (U2K)
K | 0.35 BK/WH | 372 | Remote Playback Device Audio Common Signal (U2K)
L | 0.35 OG/BK | 1406 | Remote Playback Device Left Audio Signal (UE1)
M | 0.35 L-BU | 1405 | Remote Playback Device Audio Common Signal (UE1)

### Recirculation Actuator (C60)

#### Connector Part Information

- OEM: 12059110
- Service: 88953271
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Recirculation Actuator (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 1647 | Recirculation Door Control B
B | 0.35 PK/WH | 1648 | Recirculation Door Control A

### Relay Inflatable Restraint

#### Connector Part Information

- OEM: 12110541
- Service: See Catalog
- Description: 6-Way F Metri-Pack 280 Series, Flexlock (BK)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins A1, C1 - E/A
- Core/Insulation Crimp: Pins A2, C2 - E/C
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

#### Relay Inflatable Restraint

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.5 BK | 2050 | Ground
A2 | 0.35 PK | 1139 | Ignition 1 Voltage
B1-B2 | -- | -- | Not Used
C1 | 0.5 OR/WH | 2140 | Battery Positive Voltage
C2 | 0.35 D-BU | 338 |

### Seat Adjuster Motor Assembly - Driver (AG1)

#### Connector Part Information

- OEM: 12064754
- Service: 15305872
- Description: 6-Way M Metri-Pack 280 Series Self Lock (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Adjuster Motor Assembly - Driver (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | TN | 285 | Driver Seat Horizontal Motor Forward Control
B | L-GN | 284 | Driver Seat Horizontal Motor Rearward Control
C | D-GN | 286 | Driver Seat Front Vertical Motor Up Control
D | D-BU | 287 | Driver Seat Front Vertical Motor Down Control
E | YE | 282 | Driver Seat Rear Vertical Motor Up Control
F | L-BU | 283 | Driver Seat Rear Vertical Motor Down Control

### Seat Adjuster Motor Assembly - Passenger (AG2)

#### Connector Part Information

- OEM: 12064754
- Service: 15305872
- Description: 6-Way M Metri-Pack 280 Series Self Lock (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Adjuster Motor Assembly - Passenger (AG2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | TN | 285 | Passenger Seat Horizontal Motor Forward Control
B | L-GN | 284 | Passenger Seat Horizontal Motor Rearward Control
C | D-GN | 286 | Passenger Seat Front Vertical Motor Up Control
D | D-BU | 287 | Passenger Seat Front Vertical Motor Down Control
E | YE | 282 | Passenger Seat Rear Vertical Motor Up Control
F | L-BU | 283 | Passenger Seat Rear Vertical Motor Down Control

### Seat Adjuster Switch - Driver X1 (AG1)

#### Connector Part Information

- OEM: 12015416
- Service: 12117340
- Description: 8-Way F Metri-Pack 280 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Adjuster Switch - Driver X1 (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 1040 | Battery Positive Voltage
B | YE | 282 | Driver Seat Rear Vertical Motor Up Control
C | L-BU | 283 | Driver Seat Rear Vertical Motor Down Control
D | L-GN | 284 | Driver Seat Horizontal Motor Rearward Control
E | TN | 285 | Driver Seat Horizontal Motor Forward Control
F | D-GN | 286 | Driver Seat Front Vertical Motor Up Control
G | D-BU | 287 | Driver Seat Front Vertical Motor Down Control
H | BK | 2050 | Ground

### Seat Adjuster Switch - Driver X2 (AG1)

#### Connector Part Information

- OEM: 12034343
- Service: 12101821
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Adjuster Switch - Driver X2 (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 277 | Driver Seat Recline Motor Rearward Control
B | L-GN | 276 | Driver Seat Recline Motor Forward Control

### Seat Adjuster Switch - Passenger (AG2)

#### Connector Part Information

- OEM: 12064998
- Service: 15306189
- Description: 8-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Adjuster Switch - Passenger (AG2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 1040 | Battery Positive Voltage
B | L-BU | 283 | Passenger Seat Rear Vertical Motor Down Control
C | YE | 282 | Passenger Seat Rear Vertical Motor Up Control
D | BK | 2050 | Ground
E | D-BU | 287 | Passenger Seat Front Vertical Motor Down Control
F | D-GN | 286 | Passenger Seat Front Vertical Motor UP Control
G | L-GN | 284 | Passenger Seat Horizontal Motor Rearward Control
H | TN | 285 | Passenger Seat Horizontal Motor Forward Control

### Seat Belt Buckle - Driver

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 2151 | Low Reference
B | 0.35 BK/WH | 238 | Seat Belt Switch - Left

### Seat Belt Buckle - Passenger X1

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Passenger X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 2151 | Ground
B | 0.35 BK/WH | 2484 | Seat Belt Switch - Right

### Seat Belt Buckle - Passenger X2

#### Connector Part Information

- OEM: 12110293
- Service: 12117025
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Passenger X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-BU | 5612 | 5-Volt Reference
B | 0.35 TN | 5613 | Low Reference
C | 0.35 PU | 5611 | Seat Belt Tension Sensor Signal

### Seat Belt Pretensioner - Driver

#### Connector Part Information

- OEM: 13660162
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Seat Belt Pretensioner - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK/WH | 2118 | Seat Belt Pretensioner - Left - High Control
B | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control

### Seat Belt Pretensioner - Passenger

#### Connector Part Information

- OEM: 13660163
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Seat Belt Pretensioner - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control (Regular/Crew Cab)
0.5 BK/WH | 2118 | Seat Belt Pretensioner - Right - High Control (Extended Cab)
B | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control (Regular/Crew Cab)
0.5 OG/BK | 2119 | Seat Belt Pretensioner - Right - Low Control (Extended Cab)

### Seat Lumbar Adjuster Switch - Driver (AG1)

#### Connector Part Information

- OEM: 12045688
- Service: 12101827
- Description: 8-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Lumbar Adjuster Switch - Driver (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | 2050 | Ground
B | PK | 1501 | Driver Heated Seat High/Low Signal
C | BN | 141 | Ignition Voltage
D | -- | -- | Not Used
E | BK | 2050 | Ground
F | D-BU | 611 | Driver Seat Lumbar Motor Forward Control
G | PK | 610 | Driver Seat Lumbar Motor Rearward Control
H | OG | 1040 | Battery Positive Voltage

### Seat Lumbar Adjuster Switch - Passenger (AG2)

#### Connector Part Information

- OEM: 12045688
- Service: 12101827
- Description: 8-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Lumbar Adjuster Switch - Passenger (AG2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | 2050 | Ground
B | PK | 1501 | Passenger Heated Seat High/Low Signal
C | BN | 141 | Ignition Voltage
D | RD | 1362 | Seat Belt Switch - Right
E | BK | 2050 | Ground
F | D-BU | 611 | Driver Seat Lumbar Motor Forward Control
G | PK | 610 | Passenger Seat Lumbar Motor Rearward Control
H | OG | 2240 | Battery Positive Voltage

### Seat Lumbar Motor - Driver (AR9)

#### Connector Part Information

- OEM: 12034343
- Service: 12101821
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Lumbar Motor - Driver (AR9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | 611 | Driver Seat Lumbar Motor Forward Control
B | PK | 610 | Driver Seat Lumbar Motor Rearward Control

### Seat Lumbar Motor - Passenger (AR9)

#### Connector Part Information

- OEM: 12034343
- Service: 12101821
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Lumbar Motor - Passenger (AR9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | 611 | Passenger Seat Lumbar Motor Forward Control
B | PK | 610 | Passenger Seat Lumbar Motor Rearward Control

### Seat Vertical Motor - Driver (AG1)

#### Connector Part Information

- OEM: 12129081
- Service: 12129081
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Vertical Motor - Driver (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 277 | Driver Seat Recline Motor Rearward Control
B | L-GN | 276 | Driver Seat Recline Motor Forward Control

### Secondary Air Injection (AIR) Pump (K18)

#### Connector Part Information

- OEM: 12147067
- Service: 89046640
- Description: 2-Way F Metri-Pack 630 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12147474/24
- Core/Insulation Crimp: G/F/3
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Secondary Air Injection (AIR) Pump (K18)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 5 RD | 78 | Air Pump Control
B | 5 BK | 350 | Ground

### Secondary Air Injection (AIR) Pump Relay (K18)

#### Connector Part Information

- OEM: 15336745
- Service: 15306331
- Description: 4-Way F GT 280 Metri-Pack 800 Series Sealed (GY)

#### Terminal Part Information

- Pins: 30, 87
- Terminal/Tray: 15336748/20
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

- Pins: 85, 86
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Secondary Air Injection (AIR) Pump Relay (K18)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | 5 RD | 78 | Air Pump Control
85 | 0.5 BN | 436 | Air Pump Relay Control
86 | 0.5 PK | 439 | Ignition Voltage
87 | 5 RD | 78 | Air Pump Control

### Secondary Air Injection (AIR) Pump Solenoid (K18)

#### Connector Part Information

- OEM: 13539171
- Service: See Catalog
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Secondary Air Injection (AIR) Pump Solenoid (K18)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU/WH | 6785 | Low Reference
2 | 0.5 YE | 6787 | Air Injection Reaction Control Valve Signal
3 | 0.5 BN/WH | 6789 | 5-Volt Reference
4 | 0.5 BK | 550 | Ground
5 | -- | -- | Not Used
6 | 0.8 PK/BK | 415 | Secondary Air Injection Solenoid Control

### Speaker - Left Front

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 118 | Left Front Speaker Output (-)
B | 0.5 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Front Tweeter (UQ2)

#### Connector Part Information

- OEM: 15427362
- Service: 88987841
- Description: 2-Way M 090 II (WH)

#### Terminal Part Information

- Terminal/Tray: 15305100/19
- Core/Insulation Crimp: A/E/A
- Release Tool/Test Probe: 12094429/J-35616-19 (BK)

#### Speaker - Left Front Tweeter (UQ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 118 | Left Front Speaker Output (-)
2 | 0.5 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Rear (Extended/Crew Cab)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Rear (Extended/Crew Cab)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 116 | Left Rear Speaker Output (-)
B | 0.5 BN | 199 | Left Rear Speaker Output (+)

### Speaker - Right Front

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 117 | Right Front Speaker Output (-)
B | 0.5 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Front Tweeter (UQ2)

#### Connector Part Information

- OEM: 15427362
- Service: 88987841
- Description: 2-Way M 090 II (WH)

#### Terminal Part Information

- Terminal/Tray: 15305100/19
- Core/Insulation Crimp: A/E/A
- Release Tool/Test Probe: 12094429/J-35616-19 (BK)

#### Speaker - Right Front Tweeter (UQ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 117 | Right Front Speaker Output (-)
2 | 0.5 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Rear (Extended/Crew Cab)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Right Rear (Extended/Crew Cab)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 115 | Right Rear Speaker Output (-)
B | 0.5 BN | 46 | Right Rear Speaker Output (+)

### Starter X1

#### Connector Part Information

- OEM: 12089916
- Service: 12101763
- Description: 1-Way Metri-Pack 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Starter X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 5 PU | 6 | Starter Solenoid Crank Voltage

### Steering Wheel Position Sensor

#### Connector Part Information

- OEM: 12052444
- Service: 12101874
- Description: 8-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12089660/3
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Wheel Position Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 1056 | Steering Wheel Position Sensor 5-Volt Reference
2 | 0.35 BK | 1835 | Low Reference
3 | 0.35 L-GN | 1763 | Steering Wheel Position Signal A
4 | 0.35 L-BU | 1764 | Steering Wheel Position Signal B
5 | 0.35 WH | 1765 | Steering Wheel Position Marker Pulse Signal
6 | 0.35 L-BU | 1059 | Steering Wheel Position Sensor Signal
7 | 0.35 BN | 441 | Ignition Voltage
8 | 0.35 BK/WH | 1151 | Ground

### Stop Lamp Switch

#### Connector Part Information

- OEM: 12105252
- Service: 88987863
- Description: 4-Way F 250 Series 58M (BK)

#### Terminal Part Information

- Pins: 1, 2
- Terminal/Tray: 7116-2876/10
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Stop Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 OG | 140 | Battery Positive Voltage
2 | 0.8 L-BU | 20 | Stop Lamp Control
3-4 | -- | -- | Not Used

### Stop Lamp - Left

#### Connector Part Information

- OEM: 16530669
- Service: See Catalog
- Description: 3-Way F (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Stop Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | -- | Stop Lamp Control
B | BN | -- | Park Lamp Control
G | BK | -- | Ground

### Stop Lamp - Right

#### Connector Part Information

- OEM: 16530669
- Service: See Catalog
- Description: 3-Way F (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Stop Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | -- | Stop Lamp Control
B | BN | -- | Park Lamp Control
G | BK | -- | Ground

### Sunroof Motor (CF5)

#### Connector Part Information

- OEM: 7283-5909-40
- Service: 88988798
- Description: 10-Way F 1.5 Series Unsealed (L-GY)

#### Terminal Part Information

- Pins: 1-3, 5-6, 10
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Sunroof Motor (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/PU | 1150 | Ground
2 | BN | 128 | Low Reference
3 | PU | 1353 | RAP Control
4 | -- | -- | Not Used
5 | WH | 100 | Sunroof Switch Open Signal
6 | YE/RD | 1840 | Battery Positive Voltage
7-9 | -- | -- | Not Used
10 | L-BU | 110 | Sunroof Switch Close Signal

### Sunroof Switch (CF5)

#### Connector Part Information

- OEM: 12191825
- Service: 15306048
- Description: 8-Way F GT 280 Series Unsealed (BN)

#### Terminal Part Information

- Pins: A-C, F-G
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Sunroof Switch (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | 128 | Low Reference
B | BN/WH | 230 | Instrument Panel Lamps Dimming Control
C | BK | 1350 | Ground
D-E | -- | -- | Not Used
F | OG | 110 | Sunroof Switch Close Signal
G | BN | 100 | Sunroof Switch Open Signal
H | -- | -- | Not Used

### Throttle Body

#### Connector Part Information

- OEM: 15418497
- Service: See Catalog
- Description: 6-Way F GT 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Throttle Body

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 582 | TAC Motor Control - 2
B | 0.5 YE | 581 | TAC Motor Control - 1
C | 0.35 BK | 2752 | Low Reference
D | 0.35 D-GN | 485 | TP Sensor 1 Signal
E | 0.35 GY | 2701 | 5-Volt Reference
F | 0.35 PU | 486 | TP Sensor 2 Signal

### Theft Deterrent Module (TDM)

#### Connector Part Information

- OEM:15383337
- Service: 88988353
- Description: 5-Way F SL Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Theft Deterrent Module (TDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 PU | 1807 | Class 2 Serial Data
3 | 0.35 BK/WH | 1151 | Ground
4 | 0.35 BN | 4 | Ignition Voltage
5 | 0.35 OG | 1740 | Battery Positive Voltage

### Torque Converter Clutch (TCC) Solenoid Valve (M30)

#### Connector Part Information

- OEM: 10478128
- Service: Non-Serviceable
- Description: CBL Solenoid Valve

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Torque Converter Clutch (TCC) Solenoid Valve (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD | 839 | Ignition Voltage
B | 0.5 BK | 422 | TCC Solenoid Valve Control

### Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve (M30)

#### Connector Part Information

- OEM: 12162202
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 P2 Series (BU)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD | 839 | Ignition Voltage
B | 0.5 TN | 418 | TCC PWM Solenoid Valve Control

### Traction Control Switch

#### Connector Part Information

- OEM: 12047785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/85
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Traction Control Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 2050 | Ground
B | -- | -- | Not Used
C | 0.35 BN/WH | 1571 | Traction Control Switch Signal
D | 0.35 GY | 8 | Battery Positive Voltage

### Trailer Connector (UY7)

#### Connector Part Information

- OEM: 15354653
- Service: 15306164
- Description: 7-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: B
- Terminal/Tray: 15305232/23
- Core/Insulation Crimp: B/3
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: C,E
- Terminal/Tray: 12110853/4
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D,F,G
- Terminal/Tray: 12110847/4
- Core/Insulation Crimp: C/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Trailer Connector (UY7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-GN | 1624 | Trailer Backup Lamp Control
B | 5 BK | 1350 | Ground
C | 3 D-BU | 47 | Trailer Auxiliary Control
D | 1 D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Control
E | 3 RD | 742 | Battery Positive Voltage
F | 0.8 BN | 2109 | Trailer Park Lamp Control
G | 1 YE | 1618 | Trailer Left Rear Turn/Stop Lamp Control

### Transfer Case Encoder Motor (4WD)

#### Connector Part Information

- OEM: 15326835
- Service: 88986452
- Description: 8-Way F GT 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Transfer Case Encoder Motor (4WD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-BU/WH | 1557 | Channel A Encoder - Signal
B | 0.5 RD | 1553 | Motor Control B
C | 0.5 BK | 1552 | Motor Control A
D | -- | -- | Not Used
E | 0.35 BK | 550 | Ground
F | 0.35 YE/BK | 1558 | Channel B Encoder - Signal
G | 0.35 RD/WH | 1556 | Channel C Encoder - Signal
H | 0.35 BN/WH | 1555 | Channel P Encoder - Signal

### Transfer Case 2/4 Wheel Indicator Switch (4WD)

#### Connector Part Information

- OEM: 15327093
- Service: 88987840
- Description: 2-Way F 070 SWP Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 7116-1471/12
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-33 (YE)

#### Transfer Case 2/4 Wheel Indicator Switch (4WD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 1569 | 2WD/4WD Signal
2 | 0.35 BK | 550 | Ground

### Transfer Case Neutral Switch (4WD)

#### Connector Part Information

- OEM: 10763359
- Service: 88987929
- Description: 2-Way F SWP 070 Series Sealed (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-1471/12
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-33 (YE)

#### Transfer Case Neutral Switch (4WD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 2281 | Neutral Switch Signal
2 | 0.35 BK | 550 | Ground

### Transfer Case Shift Control Module X1 (4WD)

#### Connector Part Information

- OEM: 15383128
- Service: 88953423
- Description: 16-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 173716-1/7
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Transfer Case Shift Control Module X1 (4WD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 2050 | Ground
2 | 0.5 RD | 1553 | Motor Control B
3 | 0.5 BK | 1552 | Motor Control A
4 | 0.35 L-BU | 1296 | Axle Actuator - Control
5-6 | -- | -- | Not Used
7 | 0.35 D-GN/WH | 1559 | 4-LO Switch - Signal
8 | 0.5 OG | 1540 | Battery Positive Voltage
9 | 0.5 BK | 2050 | Ground
10 | 0.35 L-GN/BK | 1563 | 2-HI Indicator - Control
11 | 0.35 TN/BK | 1566 | 4-HI Indicator - Control
12 | 0.35 PU/WH | 1565 | 4-LO Indicator - Control
13 | 0.35 BN | 1560 | Neutral Indicator Control
14 | 0.35 L-BU | 1693 | Switch Signal Low
15-16 | -- | -- | Not Used

### Transfer Case Shift Control Module X2 (4WD)

#### Connector Part Information

- OEM: 15383127
- Service: 88953394
- Description: 20-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 173716-1/7
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Transfer Case Shift Control Module X2 (4WD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | 0.35 D-BU/WH | 1557 | Channel A Encoder - Signal
7-9 | -- | -- | Not Used
10 | 0.35 PK | 339 | Ignition Voltage
11 | 0.35 GY | 2281 | Neutral Switch Signal
12 | 0.5 BK/WH | 1695 | Axle Switch Signal
13 | 0.35 TN | 1569 | 2WD/4WD Signal
14 | 0.35 RD/WH | 1556 | Channel C Encoder - Signal
15 | 0.35 YE/BK | 1558 | Channel B Encoder - Signal
16 | 0.35 PU | 1807 | Class 2 Serial Data
17 | 0.35 BN/WH | 1555 | Channel P Encoder - Signal
18 | -- | -- | Not Used
19 | 0.35 PU | 1807 | Class 2 Serial Data
20 | 0.35 GY/BK | 1694 | 5-Volt Reference

### Transmission Control Module (TCM) (M30)

#### Connector Part Information

- OEM: 13589417
- Service: See Catalog
- Description: 49-Way F GT 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Transmission Control Module (TCM) (M30)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 418 | TCC PWM Solenoid Valve Control
2 | 0.5 L-GN | 1222 | 1-2 Shift Solenoid Valve Control
3 | 0.5 BN/WH | 6254 | Input Shaft Speed Sensor Signal
4 | -- | -- | Not Used
5 | 0.5 PU/WH | 821 | VSS High Signal
6 | 0.5 TN | 2501 | GM High Speed LAN Serial Data -
7 | 0.5 TN/WH | 2500 | GM High Speed LAN Serial Data +
8-10 | -- | -- | Not Used
11 | 0.5 BN | 4 | Ignition Voltage
12-13 | -- | -- | Not Used
14 | 0.5 WH | 687 | 3-2 Shift Solenoid Valve Control
15 | -- | -- | Not Used
16 | 0.5 L-GN/BK | 822 | VSS Low Signal
17 | 0.5 L-BU/WH | 1229 | PC Solenoid Valve Low Control
18-19 | -- | -- | Not Used
20 | 0.5 YE/BK | 1223 | 2-3 Shift Solenoid Valve Control
21-22 | -- | -- | Not Used
23 | 0.5 GY | 773 | Transmission Range Switch Signal C
24 | 0.5 PK | 1224 | Transmission Fluid Pressure Switch Signal A
25 | 0.5 TN/BK | 422 | TCC Solenoid Valve Control
26-28 | -- | -- | Not Used
29 | 0.5 BK/WH | 771 | Transmission Range Switch Signal A
30 | 0.5 BK | 452 | Low Reference
31 | 0.5 PK | 139 | Ignition Voltage
32 | 0.5 OG | 440 | Battery Positive Voltage
33 | 0.5 RD | 1226 | Transmission Fluid Pressure Switch Signal C
34 | -- | -- | Not Used
35 | 0.5 YE/BK | 1227 | TFT Sensor Signal
36 | -- | -- | Not Used
37 | 0.5 TN | 2501 | GM High Speed LAN Serial Data -
38 | 0.5 TN/WH | 2500 | GM High Speed LAN Serial Data +
39 | 0.5 WH | 776 | Transmission Range Switch Signal P
40 | 0.5 RD/BK | 1228 | PC Solenoid Valve High Control
41 | 0.5 PU/WH | 821 | VSS High Signal
42 | 0.5 L-BU | 20 | Stop Lamp Control
43 | -- | -- | Not Used
44 | 0.5 D-BU | 1225 | Transmission Fluid Pressure Switch Signal B
45 | 0.5 D-BU | 6253 | Low Reference
46 | 0.5 YE | 772 | Transmission Range Switch Signal B
47-48 | -- | -- | Not Used
49 | 0.5 BK/WH | 451 | Ground

### Turn Signal Lamp - Left Rear

#### Connector Part Information

- OEM: 16530671
- Service: See Catalog
- Description: 3-Way F (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | -- | Left Rear Turn Signal Lamps Control
B | BN | -- | Park Lamp Control
BN | -- | Park Lamp Control
G | BK | -- | Ground
BK | -- | Ground

### Turn Signal Lamp - Right Rear

#### Connector Part Information

- OEM: 16530671
- Service: See Catalog
- Description: 3-Way F (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN | -- | Right Rear Turn Signal Lamps Control
B | BN | -- | Park Lamp Control
BN | -- | Park Lamp Control
G | BK | -- | Ground
BK | -- | Ground

### Vehicle Communications Interface Module (VCIM) X1

#### Connector Part Information

- OEM: 15431362
- Service: 15306351
- Description: 16-Way F 040II (WH)

#### Terminal Part Information

- Pins: 2, 3, 6, 11
- Terminal/Tray: 15355438/20
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-12 (BU)

- Pins: 7, 16
- Terminal/Tray: 175266-5/15
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Vehicle Communications Interface Module (VCIM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN/WH | 2517 | Keypad Red LED Signal
3 | 0.35 YE/BK | 2516 | Keypad Green LED Signal
4-5 | -- | -- | Not Used
6 | 0.35 L-GN/BK | 2515 | Keypad Control
7 | 0.8 BK/WH | 1151 | Ground
8-10 | -- | -- | Not Used
11 | 0.35 D-GN/WH | 2514 | Keypad Signal
12-15 | -- | -- | Not Used
16 | 0.8 OG | 340 | Battery Positive Voltage

### Vehicle Communications Interface Module (VCIM) X2

#### Connector Part Information

- OEM: 15431365
- Service: 88952886
- Description: 12-Way F 040II (WH)

#### Terminal Part Information

- Terminal/Tray: 15355438/20
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-12 (BU)

#### Vehicle Communications Interface Module (VCIM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU | 1405 | Remote Playback Device Audio Common Signal
2 | 0.35 OG/BK | 1406 | Remote Playback Device Left Audio Signal
3-4 | -- | -- | Not Used
5 | 0.35 PU | 1807 | Class 2 Serial Data
6 | 0.35 PU | 1807 | Class 2 Serial Data
7 | -- | -- | Not Used
8 | 0.35 BARE | 2012 | Drain Wire
9 | 0.5 GY | 655 | Cellular Microphone Signal
10 | 0.5 BARE | 1705 | Drain Wire
11-12 | -- | -- | Not Used

### Vehicle Speed Sensor (VSS)

#### Connector Part Information

- OEM: 15449028
- Service: 88987978
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326266
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Vehicle Speed Sensor (VSS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN/BK | 822 | Vehicle Speed Sensor (VSS) Low Signal
B | 0.5 PU/WH | 821 | Vehicle Speed Sensor (VSS) High Signal

### Window Switch - Left Rear (Crew Cab with A31)

#### Connector Part Information

- OEM: 12105465
- Service: 88987940
- Description: 8-Way F 090 II (WH)

#### Terminal Part Information

- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 1, 2, 4, 5, 6, 7, 8 - See Terminal Repair Kit
- Core/Insulation Crimp: Pins 3 - C/A
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Window Switch - Left Rear (Crew Cab with A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
2 | 0.35 BN | 9 | Park Lamp Control
3 | 1 BK | 850 | Ground
4 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal
5 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal
6 | 2 YE | 443 | Ignition Voltage
7 | 2 BN | 669 | Power Window Motor Left Rear Down Control
8 | 2 D-BU | 668 | Power Window Motor Left Rear Up Control

### Window Switch - Right Rear (Crew Cab with A31)

#### Connector Part Information

- OEM: 12105465
- Service: 88987940
- Description: 8-Way F 090 II (WH)

#### Terminal Part Information

- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 1, 2, 4, 5, 6, 7, 8 - See Terminal Repair Kit
- Core/Insulation Crimp: Pins 3 - C/A
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Window Switch - Right Rear (Crew Cab with A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
2 | 0.35 BN | 9 | Park Lamp Control
3 | 1 BK | 850 | Ground
4 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal
5 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal
6 | 2 YE | 443 | Ignition Voltage
7 | 2 BN | 669 | Power Window Motor Left Rear Down Control
8 | 2 D-BU | 668 | Power Window Motor Left Rear Up Control

### Wheel Speed Sensor (WSS) - Left Front

#### Connector Part Information

- OEM: 15497399
- Service: 88988313
- Description: 2-Way F GT 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Wheel Speed Sensor (WSS) - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 873 | Left Front Wheel Speed Sensor Signal
B | 0.5 L-BU | 830 | 12-Volt Reference

### Wheel Speed Sensor (WSS) - Right Front

#### Connector Part Information

- OEM: 15497399
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Wheel Speed Sensor (WSS) - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 833 | Right Front Wheel Speed Sensor Signal
B | 0.5 D-GN | 872 | 12-Volt Reference

### Window Motor - Driver (A31)

#### Connector Part Information

- OEM: 15398861
- Service: 89046645
- Description: 2-Way F 062 Sealed (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-1531/27
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Window Motor - Driver (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BN | 165 | Power Window Motor Left Front Down Control
2 | 2 D-BU | 164 | Power Window Motor Left Front Up Control

### Window Motor - Passenger (A31)

#### Connector Part Information

- OEM: 15398861
- Service: 89046645
- Description: 2-Way F 062 Sealed (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-1531/27
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Window Motor - Passenger (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 D-BU | 666 | Power Window Motor Right Front Up Control
2 | 2 BN | 667 | Power Window Motor Right Front Down Control

### Window Motor - Left Rear (Crew Cab A31)

#### Connector Part Information

- OEM: 15398861
- Service: 89046645
- Description: 2-Way F 062 Sealed (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-1531/27
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Window Motor - Left Rear (Crew Cab A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BN | 669 | Power Window Motor Left Rear Down Control
2 | 2 D-BU | 668 | Power Window Motor Left Rear Up Control

### Window Motor - Right Rear (Crew Cab A31)

#### Connector Part Information

- OEM: 15398861
- Service: 89046645
- Description: 2-Way F 062 Sealed (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-1531/27
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Window Motor - Right Rear (Crew Cab A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BN | 669 | Power Window Motor Right Rear Down Control
2 | 2 D-BU | 668 | Power Window Motor Right Rear Up Control

### Windshield Washer Fluid Pump

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Windshield Washer Fluid Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD | 228 | Pump Control
B | 0.35 BK | 850 | Ground

### Windshield Wiper Motor

#### Connector Part Information

- OEM: 15487756
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, B, D - 2/1
- Core/Insulation Crimp: Pins C - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Windshield Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 PU | 92 | Windshield Wiper Motor High Speed
B | 1 D-GN | 95 | Windshield Wiper Motor Low Speed
C | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
D | 1 BK | 850 | Ground

### Yaw and Lateral Accelerometer Sensor (2WD) (JL4)

#### Connector Part Information

- OEM: 10750569
- Service:See Catalog
- Description: 6-Way F MQS Socket Housing Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 962885-5/15
- Core/Insulation Crimp: 6/6
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Yaw and Lateral Accelerometer Sensor (2WD) (JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU | 2088 | Low Reference
2 | 1 D-BU | 716 | Yaw Rate Sensor Signal
3 | 0.35 GY/BK | 1337 | 5-Volt Reference
4 | -- | -- | Not Used
5 | 0.35 OR/BK | 1057 | Low Reference
6 | -- | -- | Not Used

### Yaw and Lateral Accelerometer Sensor (4WD) (JL4)

#### Connector Part Information

- OEM: 15355474
- Service: See Catalog
- Description: 6-Way F MQS Socket Housing Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 962885-5/15
- Core/Insulation Crimp: 6/6
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Yaw and Lateral Accelerometer Sensor (4WD) (JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU | 2088 | Low Reference
2 | 1 D-BU | 716 | Yaw Rate Sensor Signal
3 | 0.35 GY/BK | 1337 | 5-Volt Reference
4 | -- | -- | Not Used
5 | 0.35 OR/BK | 1057 | Low Reference
6 | -- | -- | Not Used