SER.MANUAL UPDATE SEC.8A,B & C DELETION OF FLASH TO PASS FUSE. Oldsmobile Firenza 1988

For 1990-2009 cars

# SER.MANUAL UPDATE SEC.8A,B & C DELETION OF FLASH TO PASS FUSE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTIONS 8A, 8B AND 8C ELECTRICAL - DELETION OF FLASH TO PASS FEATURE ON CANADIAN CHEVROLET CAVALIER

#### VEHICLES AFFECTED: 1988-91 'J' MODEL

The Canadian Chevrolet Cavalier built after February 4, 1991 beginning with VIN M7174724 and M5800011 will not have the Flash To Pass feature. The 1991 Chevrolet Cavalier Service Manual and Supplement will be affected as follows:

Page Action Required ------- ------------------- 8A-10-0 Delete FTP Fuse 8A-11-0 Delete FTP Fuse 8A-11-1 Delete FTP Fuse 8A-12-1 Delete FTP Fuse and circuit 740.8 orange wire 8A-100-0 Delete FTP Fuse and circuit 740.8 orange wire 8A-100-1 Delete Trouble Shooting hint #5 and "Flash To Pass; ON" in system 8A-100-2 Delete "Flash To Pass" paragraph 8A-104-2 Delete FTP Fuse 8B-2 Delete "Flash To Pass" description 8C-16 Delete Fuse #9

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.