Idle Learn. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

Anytime the powertrain control module (PCM) or the battery is disconnected, the PCM loses power, or the PCM is reprogrammed, the learned idle position of the PCM is lost. The engine idle is unstable when the learned idle position is lost.

Perform the following procedure in order to return the learned idle to the correct position:

#### Manual Transmission

1. Turn OFF the ignition.
2. Restore the PCM battery feed.
3. Turn OFF the A/C controls.
4. Set the parking brake and block the drive wheels.
5. Place the transmission in Neutral.
6. Start the engine.
7. Ensure that the engine coolant temperature (ECT) is more than 80°C (176°F).
8. Allow the engine to idle for 5 minutes.
9. Turn OFF the engine for 30 seconds.