Engine Controls Connector End Views. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

Table 1: | A/C Compressor Clutch
Table 2: | Camshaft Position (CMP) Sensor
Table 3: | Crankshaft Position (CKP) Sensor A
Table 4: | Crankshaft Position (CKP) Sensor B
Table 5: | Engine Coolant Temperature Sensor
Table 6: | Evaporative Emission (EVAP) Canister Purge Valve
Table 7: | Data Link Connector (DLC)
Table 8: | Evaporative Emission (EVAP) Canister Vent Valve
Table 9: | Fuel Tank Pressure Sensor
Table 10: | Rough Road (G) Sensor
Table 11: | Idle Air Control (IAC) Valve
Table 12: | Knock Sensor
Table 13: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1
Table 14: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2
Table 15: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1
Table 16: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2
Table 17: | Fuel Injector #1
Table 18: | Fuel Injector #2
Table 19: | Fuel Injector #3
Table 20: | Fuel Injector #4
Table 21: | Fuel Injector #5
Table 22: | Fuel Injector #6
Table 23: | Fuel Injector #7
Table 24: | Fuel Injector #8
Table 25: | Manifold Absolute Pressure (MAP) Sensor
Table 26: | Throttle Position (TP) Sensor
Table 27: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Table 28: | Vehicle Speed Sensor (VSS)
Table 29: | Ignition Control Module C1
Table 30: | Ignition Control Module C2
Table 31: | Ignition Control Module C3
Table 32: | Ignition Control Module C4

#### A/C Compressor Clutch

Connector Part Information

• | 1216-2017

• | 2-Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 450 | A/C Compressor Clutch Ground
B | DK GRN | 59 | A/C Compressor Clutch Control

#### Camshaft Position (CMP) Sensor

Connector Part Information

• | 12162196

• | 2-Way F Metri-Pack 150.2 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK/BLK | 632 | Cam Low
B | BRN/WHT | 633 | Cam High

#### Crankshaft Position (CKP) Sensor A

Connector Part Information

• | 12186884

• | 2-Way F Metri-Pack 150 Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 574 | Crankshaft Position A Low
B | YEL | 573 | Crankshaft Position Sensor A High

#### Crankshaft Position (CKP) Sensor B

Connector Part Information

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 645 | Crank B Low
B | LT BLU | 646 | Crank B High

#### Engine Coolant Temperature Sensor

Connector Part Information

• | 1211-0192

• | 3-Way F Metri-Pack 150 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 407 | Engine Coolant Temperature (ECT) Sensor Ground
B | YEL | 418 | Engine Coolant Temperature (ECT) Sensor Signal
C | DK GRN | 135 | Engine Coolant Temperature (ECT) Sensor Output

#### Evaporative Emission (EVAP) Canister Purge Valve

Connector Part Information

• | 1205-2643

• | 2-Way Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 239 | Ignition Feed
B | DK GRN/WHT | 428 | EVAP Canister Purge Valve Control

#### Data Link Connector (DLC)

Connector Part Information

• | 12110250

• | 16-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | DK GRN | 1849 | Serial Data Line - Class 2
3 | -- | -- | Not Used
4 | BLK | 1650 | Ground
5 | BLK | 1650 | Ground
6-7 | -- | -- | Not Used
8 | BLU | 1455 | RFA Program
9-13 | -- | -- | Not Used
14 | DK GRN | 835 | E and C Bus
15 | -- | -- | Not Used
16 | ORN | 540 | Power Feed

#### Evaporative Emission (EVAP) Canister Vent Valve

Connector Part Information

• | 1205-2643

• | 2-Way F Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 339 | Ignition Feed
B | WHT | 1310 | EVAP Canister Vent Valve Control

#### Fuel Tank Pressure Sensor

Connector Part Information

• | 1205-9595

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 720 | Fuel Sensor Ground
B | DK GRN | 890 | Fuel Tank Pressure Signal
C | GRY | 474 | 5V Sensor Feed

#### Rough Road (G) Sensor

Connector Part Information

• | 1212-9946

• | 3-Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | RRS3 | Rough Road Sensor Ground
B | RED | RRS1 | Rough Road Sensor Signal
C | GRY | RRS2 | Rough Road 5V Reference

#### Idle Air Control (IAC) Valve

Connector Part Information

• | 1216-2190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | Idle Air Control (IAC) Valve Coil B Signal - Low
B | LT GRN/WHT | 1749 | Idle Air Control (IAC) Valve Coil B Signal - High
C | LT BLU/BLK | 1748 | Idle Air Control (IAC) Valve Coil A Signal - Low
D | LT BLU/WHT | 1747 | Idle Air Control (IAC) Valve Coil A Signal - High

#### Knock Sensor

Connector Part Information

• | 1216800

• | 1-Way F Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 496 | Knock Sensor Signal

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1

Connector Part Information

• | 1216-0825

• | 4-Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1653 | Heated Oxygen Sensor (HO2S) - Low
B | PPL/WHT | 1665 | Heated Oxygen Sensor (HO2S) - High
C | BLK | 451 | Ground
D | PNK | 539 | Ignition Feed

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2

Connector Part Information

• | 1216-0825

• | 4-Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | Heated Oxygen Sensor (HO2S) - Low
B | PPL/WHT | 1668 | Heated Oxygen Sensor (HO2S) - High
C | BLK | 451 | Ground
D | PNK | 539 | Ignition Feed

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1

Connector Part Information

• | 1216-0825

• | 4-Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 1667 | Heated Oxygen Sensor (HO2S) - Low
B | PPL | 1666 | Heated Oxygen Sensor (HO2S) - High
C | BLK | 451 | Ground
D | PNK | 539 | Ignition Feed

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2

Connector Part Information

• | 1216-0825

• | 4-Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 1671 | LR Heated Oxygen Sensor (HO2S) - Low
B | PPL | 1670 | LR Heated Oxygen Sensor (HO2S) - High
C | BLK | 451 | Ground
D | PNK | 539 | Ignition Feed

#### Fuel Injector #1

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 739 | Injection Feed
B | BLK | 1744 | Fuel Injector #1 Control

#### Fuel Injector #2

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1239 | Injection Feed
B | LT GRN/BLK | 1745 | Fuel Injector #2 Control

#### Fuel Injector #3

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1239 | Injection Feed
B | PNK/BLK | 1746 | Fuel Injector #3 Control

#### Fuel Injector #4

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 739 | Injection Feed
B | LT BLU/BLK | 844 | Fuel Injector #4 Control

#### Fuel Injector #5

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1239 | Injection Feed
B | BLK | 845 | Fuel Injector #5 Control

#### Fuel Injector #6

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 739 | Injection Feed
B | YEL/BLK | 846 | Fuel Injector #6 Control

#### Fuel Injector #7

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 739 | Injection Feed
B | RED/BLK | 877 | Fuel Injector #7 Control

#### Fuel Injector #8

Connector Part Information

• | 1212-9140

• | 2-Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1239 | Injection Feed
B | DK BLU/WHT | 878 | Fuel Injector #8 Control

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information

• | 1212-9946

• | 3-Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 487 | Manifold Absolute Pressure (MAP) Sensor Ground
B | LT GRN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | GRY | 416 | Manifold Absolute Pressure (MAP) Sensor 5.0V Reference

#### Throttle Position (TP) Sensor

Connector Part Information

• | 1211-0192

• | 3-Way F Metri-Pack 150 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 596 | Throttle Position (TP) Sensor 5V Reference
B | BLK | 452 | Sensor Ground
C | DK BLU | 417 | Throttle Position (TP) Sensor Signal

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Connector Part Information

• | 15305555

• | 5-Way F GT 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 719 | Intake Air Temperature (IAT) Sensor Ground
B | TAN | 472 | Intake Air Temperature (IAT) Sensor Signal
C | BLK | 451 | Mass Air Flow Sensor Ground
D | PNK | 539 | Ignition Feed
E | YEL | 492 | Mass Air Flow (MAF) Sensor Signal

#### Vehicle Speed Sensor (VSS)

Connector Part Information

• | 1216-2195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 822 | Vehicle Speed Sensor (VSS) Signal - Low
B | PPL/WHT | 821 | Vehicle Speed Sensor (VSS) Signal - High

#### Ignition Control Module C1

Connector Part Information

• | 12162857

• | 6-Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 573 | Crankshaft Position (A) Sensor Signal
B | PPL | 574 | Crankshaft Position (A) Sensor Return
C-D | -- | -- | Not Used
E | RED | 645 | Crankshaft Position (B) Sensor Return
F | LT BLU | 646 | Crankshaft Position (B) Sensor Signal

#### Ignition Control Module C2

Connector Part Information

• | 12162185

• | 3-Way F Metri-Pack 150.2 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1451 | Ground
B | -- | -- | Not Used
C | PNK | 239 | Ignition Feed

#### Ignition Control Module C3

Connector Part Information

• | 12162279

• | 3-Way F Metri-Pack 150.2 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 633 | Camshaft Position Sensor Signal
B | PNK/BLK | 632 | Camshaft Position Sensor Return
C | -- | -- | Not Used

#### Ignition Control Module C4

Connector Part Information

• | 12162261

• | 2-Way F Metri-Pack 150.2 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLU/BLK | 647 | 24X Spark Reference
B | BLK | 638 | Camshaft
C | PPL/WHT | 438 | 4X Fuel Control
D | TAN/BLK | 424 | Bypass
E | WHT | 423 | Ignition Control
F | RED/BLK | 453 | Reference Low