Engine Controls Components. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Clutch Diode | Front of the engine compartment, near the A/C compressor connector | -- | --
A/C Compressor Clutch | Front of the engine | -- | Engine Controls Connector End Views in 4.0L Engine Controls
A/C Compressor Relay | Fuse/relay center box 3 | -- | --
Camshaft Position (CMP) Sensor | Front of the engine, near the power steering pump | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Crankshaft Position (CKP) Sensors A and B | Left side of the engine | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Data Link Conn (DLC) | Right side kick panel of the passenger compartment | -- | --
Engine Cooling Fans | Behind the radiator | -- | --
Engine Cooling Fan Relays | Fuse/relay center box 1 | -- | --
Engine Coolant Temperature (ECT) Sensor | Right rear of the engine on the cylinder head | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Evaporative Emission (EVAP) Canister Purge Solenoid Valve | On the right center of the engine, mounted to the manifold | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Evaporative Emission (EVAP) Canister Vent Solenoid Valve | On the top of the canister, at the left rear of the vehicle behind the rear bumper | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Fuel Injectors | Mounted on the intake manifold, part of the fuel rail | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Fuel Pump Relay | Fuse/relay center box 3 | -- | --
Fuel Sending Unit | In the fuel tank | Engine Controls Component Views in 4.0L Engine Controls | --
Fuel Tank Unit | At the rear of the vehicle | -- | --
Generator | On the front left side of the engine | -- | --
Heated Oxygen Sensor Bank 1, Sensor 1 | Mounted in the right exhaust pipe | Engine Controls Component Views in 4.0L Engine Controls | --
Heated Oxygen Sensor Bank 1, Sensor 2 | At the rear of the right catalytic converter | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Heated Oxygen Sensor Bank 2, Sensor 1 | Mounted in the left exhaust manifold | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Heated Oxygen Sensor Bank 2, Sensor 2 | At the rear of the left catalytic converter | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Idle Air Control (IAC) Valve | On the left rear of the engine, on the throttle body | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Ignition Control Coils/Module | On the right cam cover | Engine Controls Component Views in 4.0L Engine Controls | --
Instrument Cluster | On the left side of the IP | -- | --
Intake Air Temperature (IAT) Sensor | Part of Mass Air Flow Sensor | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Knock Sensor | At the center of the engine, under the intake manifold | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Manifold Absolute Pressure (MAP) Sensor | Mounted to the left side of the intake manifold by the throttle body | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Manual Transmission | At the rear of the vehicle | -- | --
Mass Air Flow (MAF) Sensor | Mounted on the air duct, in back of the intake manifold on the right side | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Powertrain Control Module (PCM) | At the right front of the passenger compartment, behind the fuse/relay center | Engine Controls Component Views in 4.0L Engine Controls | Powertrain Control Module Connector End Views in 4.0L Engine Controls
Radio | In the center of the IP, above the HVAC control | -- | --
Throttle Position (TP) Sensor | Mounted to the front of the throttle body | Engine Controls Component Views in 4.0L Engine Controls | Engine Controls Connector End Views in 4.0L Engine Controls
Vehicle Speed Sensor | On the rear left side of the transaxle | -- | Engine Controls Connector End Views in 4.0L Engine Controls