INFO ON INCORRECT PAINT CODES ON SPID LABELS. Oldsmobile Toronado 1992

For 1990-2009 cars

# INFO ON INCORRECT PAINT CODES ON SPID LABELS

#### SUBJECT: INCORRECT PAINT CODES ON SERVICE PART IDENTIFICATION LABELS

#### MODELS/YEARS: 1992 TORONADO/TROFEO'

Some vehicles produced at the Hamtramck Assembly Plant have incorrect paint codes printed on the Service Parts identification label, located in the rear compartment area of the car. Colors involved include:

GM Oldsmobile Incorrect Correct Paint Code Paint Name Label Code Label Code ---------------------------------------------------- 93U White Diamond 9097 8933 33U Driftwood Metallic - 5322

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.