WIRE WHEEL COVERS P/N FOR WHEEL COVER AND LOCK. Oldsmobile Toronado 1984

For 1990-2009 cars

# WIRE WHEEL COVERS P/N FOR WHEEL COVER AND LOCK

#### MODELS/YEARS 1984 MODELS

The custom locking wire wheel cover package (Option N91) is shipped in the trunk compartment. This package contains the locking wire wheel covers, lock brackets, lock bolts, medallions, lock key wrench and I.D./Registration Card. The standard wheel lug nuts are installed on the wheel and the twelve (12) special lug nuts are placed in the trunk compartment in a separate plastic bag. In some cases special nuts may be installed at the assembly plant.

At the time of delivery of a new vehicle by the carrier, the contents of the package containing Option N91 are to be inspected for missing or incorrect parts.

In addition, the trunk compartment is to be inspected for the plastic bag containing the special lug nuts.

Any discrepancies are to be noted on the delivery receipt and a transportation claim is to be filed for any missing or incorrect parts.

REPLACEMENT OF MISSING, INCORRECT OR LOST PARTS

Lock key wrenches and/or ID Registration Cards, are available from Norris Industries and Thompson Industries.

A. Lock key wrench missing upon delivery of vehicle from factory or lost at dealership after delivery.

Send I.D./Registration Card along with a check in the amount of $7.50 for the replacement lock key wrench to the applicable company.

B. I.D./Registration Card missing

Provide the applicable company with the color of the stripe on the lock key wrench, A new color coordinated I.D./Registration Card will be forwarded to the dealership.

C. Lock key wrench does not fit lock bolt.

Send lock key wrench and I.D./Registration Card to the applicable company with a letter indicating the color of the lock bolt in the center of the locking wire wheel cover. The proper lock key wrench and I.D./Registration Card will be returned to the dealership.

D. I.D./Registration Card and lock key wrench both missing.

Provide the color of the lock bolt in the center of the wire wheel cover, along with a check in the amount of $7.50 made payable to the applicable company. The proper lock key wrench and I.D./Registration Card will be forwarded to your dealership by the applicable company (Norris Industries or ITT Thompson Industries).

Thompson Industries - Locking wire wheel covers require a 'T' shaped lock key wrench. Their wrench will have a daub of paint to match the locknut color.

Norris Industries - Locking wire wheel covers require a 'T' shaped lock key wrench. Their wrench will have an alpha letter stamped on its cylinder portion to match the lock bolt letter.

PARTS ORDERING

All requests must be made on dealership stationary to the applicable company:

Norris Industries, Inc. Automotive Trim Division All Models 39600 Orchard Hill Place Novi, MI 48050

or

Thompson Industries 423 N. Mill Street 1984 Cutlass Supreme Adel, GA 31620 Models Only

or

Thompson Industries P.O. Box 119 All Models except Madison, FL 32340 Cutlass Supreme

Other missing or incorrect part(s) such as a locking wire wheel cover(s), lock bracket(s), medallion(s) and special lug nut(s) are available through WDDGM. See Fig. 1 for parts illustration.

Locking Wire Wheel Components

Cover Asm. Emblem Lock Bracket Special Model Norris ITT Norris ITT Norris ITT Flanged Nut ----- ------ --- ------ --- ------ --- ------------

Firenza 22515624 22520008 22515701 10017687 Omega 22515622 22520008 22515623 10017687 Cutlass Ciera Gas 14" 22515625 22520008 22515623 10017687 Diesel 22515625 22520008 22518787 10017687 Cutlass 22522275 22519903 22512339 22519904 14035642 22519905 10017687 Supreme 22522276 22515281 22512339 88 22511787 22510766 22511788 22510417 22522183 22510765 22506314 Custom Cruiser 22510766 22510417 22522183 22510765 22506315 98 Regency22524159 22524160 14035642 22506315 & Bro. Sedan Toronado 22509520 22506015 01617759 10017687

In addition to individual components, a compelte locking wire wheel package (Option N91) is available by Norris through WDDGM for the 1984 models. This package contains the following components: Four (4) locking wire wheel covers, four (4) medallions, four (4) lock brackets, four (4) lock bolts, four (4) valve extensions, (12) lug nuts, one (1) key wrench, one (1) Registration Card and Installation Instructions. Listed below are the part numbers for this package. (Thompson Industries does not package a complete a wire wheel package for service.)

WDDGM PART NUMBER MODEL ----------- ----- 997097 Toronado 998389 88 (15 x 7 wheel) 998390 98 & WK9 (15 X 6 wheel) 997784 Cutlass Ciera & Omega " 13" wheel 997785 Cutlass Ciera 14" wheel 998388 Cutlass Supreme 14" wheel 997782 "J" Firenza 13 x 5" Wheel 997783 "J" Firenza 13 x 5 1/2" Wheel w/F41

When the vehicle is being made ready for delivery, the lock brackets are to be installedd prior to installation of the wire wheel cover and medallions.

1. Raise vehicle with lift equipment.

2. Remove three (3) lug nuts from each wheel for lock bracket installation - refer to illustration. Figure 1.

3. Place lock bracket on lug nut studs.

4. Install thres (3) special lug nut on each wheel to retain lock bracket and torque to specifications. LOOSE CONDITION OF LOCK BRACKET WILL BE NORMAL. WHEN LUG NUTS ARE SEATED, FRONT WHEEL STUDS WILL HAVE A RECESSED APPEARANCE, WHICH IS NORMAL.

5. Install wheel cover on wheel.

6. Tighten lock bolt with lock key wrench.

7. Snap in center medallion.

8. Install removal label to underside of deck lid next to jacking instruction label.

9. The lock key wrench is to be placed in the glove box along with the I.D./Registration Card.

The procedure for removal and installation is to be explained to the owner prior to delivery.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.