WHEEL DISK CENTER CAP EMBLEM WARPING-REPLACE CENTER CAP. Oldsmobile Toronado 1990

For 1990-2009 cars

# WHEEL DISK CENTER CAP EMBLEM WARPING-REPLACE CENTER CAP

#### SUBJECT WHEEL CENTER CAP EMBLEM WARPING (REPLACE CENTER CAP)

#### MODELS/YEARS 1990 TORONADO AND TROFEO

Some 1990 Toronados may experience a wheel center cap emblem warping due to excessive heat generated from hard braking. Refer to the illustration below. To repair this condition replace the center cap(s) with P/N 3526685 (4 per vehicle required) which has a higher distortion temperature.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation Number: T6466 Labor Time: 0.4 hour (To Replace All Four) Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.