SEATBELT CHIMES MUTED RE-ROUTE WIRES. Oldsmobile Toronado 1981

For 1990-2009 cars

# SEATBELT CHIMES MUTED RE-ROUTE WIRES

SEAT BELT CHIMES MUTED ON ELDORADOS OR SEVILLES MUTED SEAT BELT CHIMES ON 1981 E AND K CARS CAN BE CAUSED BY THE CB RADIO ANTENNA SPLITTER WIRE BEING ROUTED ACROSS THE CHIME. RE-ROUTE TO AVOID CONTACT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.