SLIPPAGE 1-2 UPSHIFT RESULTING FROM PUMP SEAL RINGS. Pontiac Acadian (Canada) 1980

For 1990-2009 cars

# SLIPPAGE 1-2 UPSHIFT RESULTING FROM PUMP SEAL RINGS

SOME 1980-81 CHEVETTES MAY EXPERIENCE SLIPPAGE ON THE 1-2 UP SHIFT WHICH FEELS LIKE THE TRANSMISSION IS IN NEUTRAL. THIS CONDITION COULD BE CAUSED BY A WORN SECOND GEAR CLUTCH OIL SEAL RING. SINCE THE WEAR PATTERN IS DIFFICULT TO SEE ON THE PUMP, THE RING SHOULD BE REMOVED FOR INSPECTION AND REPLACED IF NECESSARY. ILLUSTRATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.