REDUCTION GEAR RATTLE NOISE REPLACE INPUT GEAR. Pontiac Acadian (Canada) 1986

For 1990-2009 cars

# REDUCTION GEAR RATTLE NOISE REPLACE INPUT GEAR

1985-86 T-1000 MODELS

#### CONDITION:

-------- A rattle may be experienced in first, second, and third gear, but not in fourth gear.

CAUSE/CORRECTION: ---------------- This condition may be repaired by replacing the input qear, part number 14024970.

SERVICE DEPARTMENT PONTIAC DIVISION GENERAL MOTORS CORPORATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.