POOR DRIVEABILITY CONDITIONS NEW PROM AVAIL.(P/N 1226587). Pontiac J2000 1983

For 1990-2009 cars

# POOR DRIVEABILITY CONDITIONS NEW PROM AVAIL.(P/N 1226587)

THERE HAVE BEEN SOME COMMENTS OF VEHICLES EQUIPPED WITH THE 1.8L EFI AND 5-SPEED TRANSMISSION ENCOUNTERING A CLOSED THROTTLE STALLING CONDITION. THIS CONDITION OCCURS AFTER A CLOSED THROTTLE COAST DOWN FROM HIGHWAY SPEEDS AND DEPRESSING THE CLUTCH PEDAL AT APPROXIMATELY 35 MILES PER HOUR. IF THIS CONDITION IS ENCOUNTERED, REPLACE THE PROM WITH PART NUMBER 1226587.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.