SUN VISOR LOOSE/WILL NOT HOLD POSITION (INSTALL SLEEVE). Pontiac Safari Wagon 1987

For 1990-2009 cars

# SUN VISOR LOOSE/WILL NOT HOLD POSITION (INSTALL SLEEVE)

SUN VISOR LOOSE AND WILL NOT HOLD POSITION

#### Models Affected: 1986-88 PARISIENNE/SAFARI WAGONS

Owner comments on Parisienne/Safari model sun visors that are loose and will not hold position can be addressed by replacing the sleeve, P/N 8740843 with a new thicker sleeve, P/N 17927383.

1. Loosen tensioning screw and remove sunshade from support.

2. Extract clear plastic sleeve from sunshade using needle nose pliers and replace with new sleeve (black plastic), P/N 17927383.

3. Check rod on support assembly to be sure it does not turn within the support. If rod turns replace support assembly.

4. Reinstall sunshade and check for proper operation.

#### Warranty Information:

Labor Operation: T1370

Labor Time : .3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.