INFORMATION ON SPECIAL TOOL FOR HEADLAMP AIMING. Saturn Saturn 1993

For 1990-2009 cars

# INFORMATION ON SPECIAL TOOL FOR HEADLAMP AIMING

#### SUBJECT: Information on Special Tool for Headlamp Aiming

#### MODELS AFFECTED: All 1991-1993 Saturns

PURPOSE: Enclosed is one Headlamp Aiming Spacer Kit (SA9302NE) to be used with the Hopkins Small Universal Adapters which are supplied with the Hopkins Mechanical Aimer. This aiming kit is used when mechanically aiming Saturn composite headlamps that are used on the SL, SL1, SL2 Sedans, SCI Coupes and SW1, SW2 Station Wagons.

It is important to note that the Hopkins Small Universal Adapters, with the spacers installed, can be used to aim the retractable headlamps on the SC and SC2 Coupes. The setting on the adjustment rods must incorporate the added length of the spacer.

This Headlamp Aiming Spacer Kit replaces the currently released Headlamp Aim Adapter Package (P/N 21020533) which will be discontinued.

When mechanically aiming Saturn headlamps, please refer to the instruction sheet enclosed with the Headlamp Aiming Spacer Kit or to the "Headlamp Aiming" procedure in the "Front End" section of the 1991-1993 Body/Collision Repair Service Manual" due to be printed in March, 1993.

Additional sets of the Headlamp Aiming Spacer Kit may be obtained from the OTC division of SPX Corporation (P/N SA9302NE).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.