SERVICE INFO. ON REMOVAL OF I/P UPPER TRIM PANEL. Saturn Saturn 1995

For 1990-2009 cars

# SERVICE INFO. ON REMOVAL OF I/P UPPER TRIM PANEL

#### SUBJECT: Service Information on Removal of I/P Upper Trim Panel Assembly

#### MODELS AFFECTED: 1995 Saturns

PURPOSE: During removal of the I/P upper trim panel assembly, the I/P upper trim panel assembly may catch on the VIN plate, making removal difficult.

PROCEDURE: To prevent the VIN plate from contacting the I/P upper trim panel assembly during removal, insert a trim tool or putty knife at the front of the VIN plate so that when you pull rearward, the panel will ride up and over the VIN plate.

#### IMPORTANT: Use care so no damage is done to VIN plate or I/P upper trim panel assembly.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.