Service Manual Update for Specifications in the 1991-1992 Body/Collision Service Manual. Saturn Saturn 1992

For 1990-2009 cars

# Service Manual Update for Specifications in the 1991-1992 Body/Collision Service Manual

Subject: | 1991 -- 1992 Body/Collision Repair, and Specifications Service Manual Updates (Headlamp Cover Panel Assembly Gap Specifications)

Models: | All 1991-1992 Saturn SC Coupes

### Purpose:

The 1991-1992 Body/Collision Repair and 1991-1992 Revised Specifications Service Manual were published without the gap specifications for the headlamp cover panel assembly for the Saturn SC Coupe.

Please add the following gap specifications to page BDGI 40 in the General Information section of the 1991-1992 Body/Collision Repair Service Manual and to page RFSP 64 of the 1991-1992 Revised Specifications Service Manual.

Location | Clearance Gap mm (in) | Flushness mm (in)
--- | --- | ---
Headlamp cover panel assembly to hood | 6.0+/-1.0 parallel within 1.0 (0.24+/- 0.04 parallel within 0.24) | +0.0/-1.0 (+0.0/-0.04
Headlamp cover panel assembly to fender | 5.0+/-1.0 parallel within 1.0 (0.20+/-0.04 parallel within 0.24) | +0.75/-1.75 (+0.03/-0.07)