SER. MAN. UPDATE SEC. SIR-REV. TORQUE SPEC.-INFLATOR MODULE. Saturn Saturn 1992

For 1990-2009 cars

# SER. MAN. UPDATE SEC. SIR-REV. TORQUE SPEC.-INFLATOR MODULE

#### SUBJECT: Supplemental Inflatable Restraint System Service Manual Update (Revised Torque Specification for Inflator Module [Air Bag] Attachment Bolts)

#### PURPOSE:

The 1992-1/2 "Supplemental Inflatable System Service Manual" has an incorrect torque specification for the inflator module (air bag) in "Section 3 - Service."

#### PROCEDURE:

Please change the torque specification from 12 N-m (106 lbs. in.) to 10 N-m (88 lbs. in.) in the following steps.

PAGE NUMBER STEP NUMBER ----------- ----------- 5 2 7 6 9 7

#### IMPORTANT: Always replace inflator module (air bag) fasteners. Never reuse old fasteners.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.