INFORMATION ON BRAKE LAMP FUSE RATING. Saturn Saturn 1992

For 1990-2009 cars

# INFORMATION ON BRAKE LAMP FUSE RATING

#### SUBJECT: Service Information on Brake Lamp Fuse Rating

#### MODELS AFFECTED: 1992-1994 Saturns

PURPOSE: In the "Power Distribution" section of the "1991-1994 Electrical Service Manual" the fuse rating for the BRAKE Fuse is indicated in numerous places as 20 amp for i992-1994 vehicles. This is in error. The fuse rating of the BRAYE Fuse for 1992 - 1994 vehicles is 15 amp. The BRAKE Fuse used on 1991 vehicles is 20 amp.

#### NOTICE: Using a fuse with a higher rating could cause damage to the vehicle's electrical system.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.